#
#	3GPP stuff.
#
#	ftp://ftp.3gpp.org/specs/2002-06/R1999/29_series/29061-3a0.zip
#
#	$Id: dictionary.3gpp 24293 2008-02-08 16:32:12Z etxrab $
#
VENDOR		3GPP		10415

BEGIN-VENDOR	3GPP

#
#	Most of the 'string' attributes are UTF-8 encoded text.
#	Maybe we want a UTF-8 'type' in the server...
#
ATTRIBUTE	3GPP-IMSI								1		string	
ATTRIBUTE	3GPP-Charging-ID						2		integer
ATTRIBUTE	3GPP-PDP-Type							3		integer
ATTRIBUTE	3GPP-Charging-Gateway-Address			4		ipaddr
ATTRIBUTE	3GPP-GPRS-Negotiated-QoS-profile		5		string
ATTRIBUTE	3GPP-SGSN-Address						6		ipaddr
ATTRIBUTE	3GPP-GGSN-Address						7		ipaddr
ATTRIBUTE	3GPP-IMSI-MCC-MNC						8		string
ATTRIBUTE	3GPP-GGSN-MCC-MNC						9		string
ATTRIBUTE	3GPP-NSAPI								10		string
ATTRIBUTE	3GPP-Session-Stop-Indicator				11		octets
ATTRIBUTE	3GPP-Selection-Mode						12		string
ATTRIBUTE	3GPP-Charging-Characteristics			13		string
ATTRIBUTE	3GPP-Charging-Gateway-IPv6-Address		14		ipv6addr
ATTRIBUTE	3GPP-SGSN-IPv6-Address					15		ipv6addr
ATTRIBUTE	3GPP-GGSN-IPv6-Address					16		ipv6addr
ATTRIBUTE	3GPP-IPv6-DNS-Servers					17		ipv6addr
ATTRIBUTE	3GPP-SGSN-MCC-MNC						18		string
ATTRIBUTE	3GPP-Teardown-Indicator					19		octets
ATTRIBUTE	3GGP-IMEISV								20		octets
ATTRIBUTE	3GPP-RAT-Type							21		octets
ATTRIBUTE	3GPP-User-Location-Info					22		octets
ATTRIBUTE	3GPP-MS-TimeZone						23		octets
ATTRIBUTE	3GPP-Camel-Charging-Info				24		octets
ATTRIBUTE	3GPP-Packet-Filter						25		octets
ATTRIBUTE	3GPP-Negotiated-DSCP					26		string

#
#	This attribute is really an array of IPv6 addresses.
#	Why the heck couldn't they just send multiple attributes?
#
ATTRIBUTE	3GPP-IPv6-DNS-Servers				17		octets 
ATTRIBUTE	3GPP-SGSN-MCC-MNC					18		string

# Below set to RADIUS_BINSTRING untill "proper" decoding is added ( Comment from old radius dissector ) 

ATTRIBUTE	3GPP-Teardown-Indicator				19		octets
ATTRIBUTE	3GPP-IMEISV							20		octets
ATTRIBUTE	3GPP-RAT-Type						21		octets
ATTRIBUTE	3GPP-User-Location-Info				22		octets
ATTRIBUTE	3GPP-MS-TimeZone					23		octets
ATTRIBUTE	3GPP-Camel-Charging-Info			24		octets
ATTRIBUTE	3GPP-Packet-Filter					25		octets
ATTRIBUTE	3GPP-Negotiated-DSCP				26		octets

VALUE		3GPP-PDP-Type		IPv4			0
VALUE		3GPP-PDP-Type		PPP				1
VALUE		3GPP-PDP-Type		IPv6			2
END-VENDOR	3GPP
