#
# dictionary.acc
#		Dictionary for Acc/Newbridge, models Tigris, Amazon, etc.
#		Written by Stephane Marzloff <smarzloff@carif-idf.org>
#		based on specifications available through ftp and the web.
#
# Version:	@(#)dictionary.acc  1.00  smarzloff  21-Jun-1999
#

VENDOR	Acc	5

#
# Acc specific
ATTRIBUTE	Acc-Reason-Code			1	integer		Acc
ATTRIBUTE	Acc-Ccp-Option			2	integer		Acc
ATTRIBUTE	Acc-Input-Errors		3	integer		Acc
ATTRIBUTE	Acc-Output-Errors		4	integer		Acc
ATTRIBUTE	Acc-Access-Partition		5	string		Acc
ATTRIBUTE	Acc-Customer-Id			6	string		Acc
ATTRIBUTE	Acc-Ip-Gateway-Pri		7	ipaddr		Acc
ATTRIBUTE	Acc-Ip-Gateway-Sec		8	ipaddr		Acc
ATTRIBUTE	Acc-Route-Policy		9	integer		Acc
ATTRIBUTE	Acc-ML-MLX-Admin-State		10	integer		Acc
ATTRIBUTE	Acc-ML-Call-Threshold		11	integer		Acc
ATTRIBUTE	Acc-ML-Clear-Threshold		12	integer		Acc
ATTRIBUTE	Acc-ML-Damping-Factor		13	integer		Acc
ATTRIBUTE	Acc-Tunnel-Secret		14	string		Acc
ATTRIBUTE	Acc-Clearing-Cause		15	integer		Acc
ATTRIBUTE	Acc-Clearing-Location		16	integer		Acc
ATTRIBUTE	Acc-Service-Profile		17	string		Acc
ATTRIBUTE	Acc-Request-Type		18	integer		Acc
ATTRIBUTE	Acc-Bridging-Support		19	integer		Acc
ATTRIBUTE	Acc-Apsm-Oversubscribed		20	integer		Acc
ATTRIBUTE	Acc-Acct-On-Off-Reason		21	integer		Acc
ATTRIBUTE	Acc-Tunnel-Port			22	integer		Acc
ATTRIBUTE	Acc-Dns-Server-Pri		23	ipaddr		Acc
ATTRIBUTE	Acc-Dns-Server-Sec		24	ipaddr		Acc
ATTRIBUTE	Acc-Nbns-Server-Pri		25	ipaddr		Acc
ATTRIBUTE	Acc-Nbns-Server-Sec		26	ipaddr		Acc
ATTRIBUTE	Acc-Dial-Port-Index		27	integer		Acc
ATTRIBUTE	Acc-Ip-Compression		28	integer		Acc
ATTRIBUTE	Acc-Ipx-Compression		29	integer		Acc
ATTRIBUTE	Acc-Connect-Tx-Speed		30	integer		Acc
ATTRIBUTE	Acc-Connect-Rx-Speed		31	integer		Acc
ATTRIBUTE	Acc-Modem-Modulation-Type	32	string		Acc
ATTRIBUTE	Acc-Modem-Error-Protocol	33	string		Acc
ATTRIBUTE	Acc-Callback-Delay		34	integer		Acc
ATTRIBUTE	Acc-Callback-Num-Valid		35	string		Acc
ATTRIBUTE	Acc-Callback-Mode		36	integer		Acc
ATTRIBUTE	Acc-Callback-CBCP-Type		37	integer		Acc
ATTRIBUTE	Acc-Dialout-Auth-Mode		38	integer		Acc
ATTRIBUTE	Acc-Dialout-Auth-Password	39	string		Acc
ATTRIBUTE	Acc-Dialout-Auth-Username	40	string		Acc
ATTRIBUTE	Acc-Access-Community		42	integer		Acc
ATTRIBUTE	Acc-Vpsm-Reject-Cause		43	integer		Acc
ATTRIBUTE	Acc-Ace-Token			44	string 		Acc
ATTRIBUTE	Acc-Ace-Token-Ttl		45	integer		Acc
ATTRIBUTE	Acc-Ip-Pool-Name		46	string 		Acc
ATTRIBUTE	Acc-Igmp-Admin-State		47	integer		Acc
ATTRIBUTE	Acc-Igmp-Version		48	integer		Acc

VALUE		Acc-Reason-Code		No-reason-No-Failure		0
VALUE		Acc-Reason-Code		Resource-shortage		1
VALUE		Acc-Reason-Code		Session-already-open		2
VALUE		Acc-Reason-Code		Too-many-RADIUS-users		3
VALUE		Acc-Reason-Code		No-authentification-server	4
VALUE		Acc-Reason-Code		No-authentification-response	5
VALUE		Acc-Reason-Code		No-accounting-server		6
VALUE		Acc-Reason-Code		No-accounting-response		7
VALUE		Acc-Reason-Code		Access-Denied			8
VALUE		Acc-Reason-Code		Temporary-buffer-shortage	9
VALUE		Acc-Reason-Code		Protocol-error			10
VALUE		Acc-Reason-Code		Invalid-attribute		11
VALUE		Acc-Reason-Code		Invalid-service-type		12
VALUE		Acc-Reason-Code		Invalid-framed-protocol		13
VALUE		Acc-Reason-Code		Invalid-attribute-value		14
VALUE		Acc-Reason-Code		Invalid-user-information	15
VALUE		Acc-Reason-Code		Invalid-IP-address		16
VALUE		Acc-Reason-Code		Invalid-integer-syntax		17
VALUE		Acc-Reason-Code		Invalid-NAS-port		18
VALUE		Acc-Reason-Code		Requested-by-user		19
VALUE		Acc-Reason-Code		Network-disconnect		20
VALUE		Acc-Reason-Code		Service-interruption		21
VALUE		Acc-Reason-Code		Physical-port-error		22
VALUE		Acc-Reason-Code		Idle-timeout			23
VALUE		Acc-Reason-Code		Session-timeout			24
VALUE		Acc-Reason-Code		Administrative-reset		25
VALUE		Acc-Reason-Code		NAS-reload-or-reset		26
VALUE		Acc-Reason-Code		NAS-error			27
VALUE		Acc-Reason-Code		NAS-request			28
VALUE		Acc-Reason-Code		Undefined-reason-given		29
VALUE		Acc-Reason-Code		Conflicting-attributes		30
VALUE		Acc-Reason-Code		Port-limit-exceeded		31
VALUE		Acc-Reason-Code		Facility-not-available		32
VALUE		Acc-Reason-Code		Internal-config-error		33
VALUE		Acc-Reason-Code		Bad-route-specification		34
VALUE		Acc-Reason-Code		Access-Partition-bind-failure	35
VALUE		Acc-Reason-Code		Security-violation		36
VALUE		Acc-Reason-Code		Request-type-conflict		37
VALUE		Acc-Reason-Code		Configuration-disallowed	38
VALUE		Acc-Reason-Code		Missing-attribute		39
VALUE		Acc-Reason-Code		Invalid-request			40
VALUE		Acc-Reason-Code		Missing-parameter		41
VALUE		Acc-Reason-Code		Invalid-parameter		42
VALUE		Acc-Reason-Code		Call-cleared-with-cause		43
VALUE		Acc-Reason-Code		Inopportune-config-request	44
VALUE		Acc-Reason-Code		Invalid-config-parameter	45
VALUE		Acc-Reason-Code		Missing-config-parameter	46
VALUE		Acc-Reason-Code		Incompatible-service-profile	47
VALUE		Acc-Reason-Code		Administrative-reset-2		48
VALUE		Acc-Reason-Code		Administrative-reload		49
VALUE		Acc-Reason-Code		Port-unneeded			50
VALUE		Acc-Reason-Code		Port-preempted			51
VALUE		Acc-Reason-Code		Port-suspended			52
VALUE		Acc-Reason-Code		Service-unavailable		53
VALUE		Acc-Reason-Code		Callback			54
VALUE		Acc-Reason-Code		User-error			55
VALUE		Acc-Reason-Code		Host-request			56

VALUE		Acc-Ccp-Option		Disabled			1
VALUE		Acc-Ccp-Option		Enabled				2

VALUE		Acc-Route-Policy	Funnel				1
VALUE		Acc-Route-Policy	Direct				2

VALUE		Acc-ML-MLX-Admin-State	Enabled				1
VALUE		Acc-ML-MLX-Admin-State	Disabled			2

VALUE		Acc-Clearing-Cause	Cause-unspecified		0
VALUE		Acc-Clearing-Cause	Unassigned-number		1
VALUE		Acc-Clearing-Cause	No-route-to-transit-network	2
VALUE		Acc-Clearing-Cause	No-route-to-destination		3
VALUE		Acc-Clearing-Cause	Channel-unacceptable		6
VALUE		Acc-Clearing-Cause	Call-awarded-being-delivered	7
VALUE		Acc-Clearing-Cause	Normal-clearing			16
VALUE		Acc-Clearing-Cause	User-busy			17
VALUE		Acc-Clearing-Cause	No-user-responding		18
VALUE		Acc-Clearing-Cause	User-alerted-no-answer		19
VALUE		Acc-Clearing-Cause	Call-rejected			21
VALUE		Acc-Clearing-Cause	Number-changed			22
VALUE		Acc-Clearing-Cause	Non-selected-user-clearing	26
VALUE		Acc-Clearing-Cause	Destination-out-of-order	27
VALUE		Acc-Clearing-Cause	Invalid-or-incomplete-number	28
VALUE		Acc-Clearing-Cause	Facility-rejected		29
VALUE		Acc-Clearing-Cause	Response-to-status-inquiry	30
VALUE		Acc-Clearing-Cause	Normal-unspecified-cause	31
VALUE		Acc-Clearing-Cause	No-circuit-or-channel-available	34
VALUE		Acc-Clearing-Cause	Network-out-of-order		38
VALUE		Acc-Clearing-Cause	Temporary-failure		41
VALUE		Acc-Clearing-Cause	Switching-equipment-congestion	42
VALUE		Acc-Clearing-Cause	Access-information-discarded	43
VALUE		Acc-Clearing-Cause	Circuit-or-channel-unavailable	44
VALUE		Acc-Clearing-Cause	Circuit-or-channed-preempted	45
VALUE		Acc-Clearing-Cause	Resources-unavailable		47
VALUE		Acc-Clearing-Cause	Quality-of-service-unavailable	49
VALUE		Acc-Clearing-Cause	Facility-not-subscribed		50
VALUE		Acc-Clearing-Cause	Outgoing-calls-barred		52
VALUE		Acc-Clearing-Cause	Incoming-calls-barred		54
VALUE		Acc-Clearing-Cause	Bearer-capability-unauthorized	57
VALUE		Acc-Clearing-Cause	Bearer-capability-not-available	58
VALUE		Acc-Clearing-Cause	Service-not-available		63
VALUE		Acc-Clearing-Cause	Bearer-capablity-not-implmented	65
VALUE		Acc-Clearing-Cause	Channel-type-not-implemented	66
VALUE		Acc-Clearing-Cause	Facility-not-implemented	69
VALUE		Acc-Clearing-Cause	Restrcted-digtal-infrmtion-only	70
VALUE		Acc-Clearing-Cause	Service-not-implemented		79
VALUE		Acc-Clearing-Cause	Invalid-call-reference		81
VALUE		Acc-Clearing-Cause	Identified-channel-doesnt-exist	82
VALUE		Acc-Clearing-Cause	Call-identify-in-use		84
VALUE		Acc-Clearing-Cause	No-call-suspended		85
VALUE		Acc-Clearing-Cause	Suspended-call-cleared		86
VALUE		Acc-Clearing-Cause	Incompatible-destination	88
VALUE		Acc-Clearing-Cause	Invalid-transit-network-selctin	91
VALUE		Acc-Clearing-Cause	Invalid-message			95
VALUE		Acc-Clearing-Cause	Mandtory-infrmtion-elment-miss	96
VALUE		Acc-Clearing-Cause	Message-not-implemented		97
VALUE		Acc-Clearing-Cause	Inopportune-message		98
VALUE		Acc-Clearing-Cause	Infrmtion-elemnt-not-implmented	99
VALUE		Acc-Clearing-Cause	Invlid-infrmtion-element-contnt	100
VALUE		Acc-Clearing-Cause	Message-incompatible-with-state	101
VALUE		Acc-Clearing-Cause	Recovery-on-timer-expiration	102
VALUE		Acc-Clearing-Cause	Mndtry-infrmtion-elmnt-lngt-err	103
VALUE		Acc-Clearing-Cause	Protocol-error			111
VALUE		Acc-Clearing-Cause	Interworking			127

VALUE		Acc-Clearing-Location	Local-or-remote-user		0
VALUE		Acc-Clearing-Location	Prvte-ntwork-serving-local-user	1
VALUE		Acc-Clearing-Location	Pblic-ntwork-serving-local-user	2
VALUE		Acc-Clearing-Location	Transit-network			3
VALUE		Acc-Clearing-Location	Prvte-ntwork-serv-remote-user	4
VALUE		Acc-Clearing-Location	Pblic-ntwork-serv-remote-user	5
VALUE		Acc-Clearing-Location	International-network		6
VALUE		Acc-Clearing-Location	Beyond-interworking-point	10

VALUE		Acc-Request-Type	Ring-Indication			1
VALUE		Acc-Request-Type	Dial-Request			2
VALUE		Acc-Request-Type	User-Authentification		3
VALUE		Acc-Request-Type	Tunnel-Authentification		4

VALUE		Acc-Bridging-Support	Disabled			1
VALUE		Acc-Bridging-Support	Enabled				2

VALUE		Acc-Apsm-Oversubscribed	False				1
VALUE		Acc-Apsm-Oversubscribed	True				2

VALUE		Acc-Acct-On-Off-Reason	NAS-Reset			0
VALUE		Acc-Acct-On-Off-Reason	NAS-Reload			1
VALUE		Acc-Acct-On-Off-Reason	Configuration-Reset		2
VALUE		Acc-Acct-On-Off-Reason	Configuration-Reload		3
VALUE		Acc-Acct-On-Off-Reason	Enabled				4
VALUE		Acc-Acct-On-Off-Reason	Disabled			5

VALUE		Acc-Ip-Compression	Disabled			1
VALUE		Acc-Ip-Compression	Enabled				2

VALUE		Acc-Ipx-Compression	Disabled			1
VALUE		Acc-Ipx-Compression	Enabled				2

VALUE		Acc-Callback-Mode	User-Auth			0
VALUE		Acc-Callback-Mode	User-Specified-E-164		3
VALUE		Acc-Callback-Mode	CBCP-Callback			6
VALUE		Acc-Callback-Mode	CLI-Callback			7

VALUE		Acc-Callback-CBCP-Type	CBCP-None			1
VALUE		Acc-Callback-CBCP-Type	CBCP-User-Specified		2
VALUE		Acc-Callback-CBCP-Type	CBCP-Pre-Specified		3

VALUE		Acc-Dialout-Auth-Mode	PAP				1
VALUE		Acc-Dialout-Auth-Mode	CHAP				2
VALUE		Acc-Dialout-Auth-Mode	CHAP-PAP			3
VALUE		Acc-Dialout-Auth-Mode	NONE				4

VALUE		Acc-Access-Community	PUBLIC				1
VALUE		Acc-Access-Community	NETMAN				2

#	Acc-Vpsm-Reject-Cause values (available in access-reject packets only) 
VALUE	Acc-Vpsm-Reject-Cause	No-Access-Partition             1
VALUE	Acc-Vpsm-Reject-Cause   Access-Partition-Disabled       2
VALUE	Acc-Vpsm-Reject-Cause	Partition-Portlimit-Exceeded    3
VALUE	Acc-Vpsm-Reject-Cause	License-Portlimit-Exceeded      4
VALUE	Acc-Vpsm-Reject-Cause	Home-Server-Down                5
VALUE	Acc-Vpsm-Reject-Cause	Rejected-By-Home-Server         6
VALUE	Acc-Vpsm-Reject-Cause	NAS-Administratively-Disabled   7

#	Acc-Igmp-Admin-State values 
VALUE	Acc-Igmp-Admin-State	Enabled     			1
VALUE	Acc-Igmp-Admin-State	Disabled    			2

#	Acc-Igmp-Version values 
VALUE	Acc-Igmp-Version	V1    				1
VALUE	Acc-Igmp-Version	V2   				2
