#
# Ascend dictionary.
# $Id: dictionary.ascend 14924 2005-07-15 21:03:13Z lego $
#
#		Enable by putting the line "$INCLUDE dictionary.ascend" into
#		the main dictionary file.
#
# Version:	1.00  21-Jul-1997  Jens Glaser <jens@regio.net>
#		1.01  22-Jan-1998  Tomas Pospisek <tpo@spin.ch>
#		1.2   28-Sept-2000 Chris Adams <cmadams@hiwaay.net>
#		1.3   12-Dec-2000 Miquel van Smoorenburg <miquels@cistron.nl>
#
#
#  The Ascend-Data-Filter and Ascend-Call-Filter are case insensitive
#  strings, with the following format:
#
#  IP FILTERS:
#
#	ip dir action [ dstip n.n.n.n/nn ] [ srcip n.n.n.n/nn ]
#	    [ proto [ dstport cmp value ] [ srcport cmd value ] [ est ] ] 
#
# Fields in [...] are optional.
#	where:
#
#	ip:		Keyword to designate an IP filter. Actually this
#			has been determined by parseFilter.
#
#	dir:		Filter direction. "IN" or "OUT"
#
#	action:		Filter action. "FORWARD" or "DROP"
#
#	dstip:		Keyword for destination IP address.
#			n.n.n.n = IP address. /nn - netmask. 
#			
#	srcip:		Keyword for source IP address.
#			n.n.n.n = IP address. /nn - netmask. 
#			
#	proto:		Optional protocol field. Either a name or
#			number. Known names are in FilterProtoName[].
#			
#	dstport:	Keyword for destination port. Only valid with tcp
#			or udp. 'cmp' are in FilterPortType[]. 'value' can be
#			a name or number.
#
#	srcport:	Keyword for source port. Only valid with tcp
#			or udp. 'cmp' are in FilterPortType[]. 'value' can be
#			a name or number.
#			
#	est:		Keyword for TCP established. Valid only for tcp.
#
#  IPX FILTERS
#
#  ipx dir action [ srcipxnet nnnn srcipxnode mmmmm [srcipxsoc cmd value ]]
#                 [ dstipxnet nnnn dstipxnode mmmmm [dstipxsoc cmd value ]]
#
# Fields in [...] are optional.
#	where:
#
#	ipx:		Keyword to designate an IPX filter. Actually this
#			has been determined by parseFilter.
#
#	dir:		Filter direction. "IN" or "OUT"
#
#	action:		Filter action. "FORWARD" or "DROP"
#
#	srcipxnet:      Keyword for source IPX address.
#			nnnn = IPX Node address.
#
#	srcipxnode:     Keyword for source IPX Node address.
#                  	mmmmm = IPX Node Address, could be FFFFFF.
#                  	A vlid ipx node number should accompany ipx net number.
#
#	srcipxsoc:      Keyword for source IPX socket address.
#
#	cmd:            One of ">" or "<" or "=" or "!=".
#			(without the quotes)
#
# 	value:          Socket value to be compared against, in hex. 
#			
#	dstipxnet:	Keyword for destination IPX address.
#			nnnn = IPX Node address. 
#			
#	dstipxnode:	Keyword for destination IPX Node address.
#  			mmmmm = IPX Node Address, could be FFFFFF.
#			A vlid ipx node number should accompany ipx net number.
#			
#	dstipxsoc:	Keyword for destination IPX socket address.
#			
#	cmd:		One of ">" or "<" or "=" or "!=".
#			(without the quotes)
#			
#	value:		Socket value to be compared against, in hex.
#
#  GENERIC FILTERS
#
#	generic dir action offset mask value [== or != ] [more]
#
# Fields in [...] are optional.
#	where:
#
# 	generic:	Keyword to indicate a generic filter. This
#			has been determined by parseFilter.
#
#	dir:		Filter direction. "IN" or "OUT"
#
#	action:		Filter action. "FORWARD" or "DROP"
#
#	offset:		A Number. Specifies an offset into a frame 
#			to start comparing.
#			
#	mask:		A hexadecimal mask of bits to compare.
#			
#	value:		A value to compare with the masked data.
#
#	compNeq:	Defines type of comparison. ( "==" or "!=")
#			Default is "==".
#			
#	more:		Optional keyword MORE, to represent the attachment
#			to the next entry.

VENDOR		Ascend		529

#
#	Ascend specific extensions
#	Used by ASCEND MAX/Pipeline products
#
#	This next block is renamed because they share the same
#	names as the vendor-specific attributes, BUT they occur
#	in the lower (1-255) RADIUS attribute space.
#
#	Older Ascend software will send these, rather than the
#	vendor specific attributes.
#
ATTRIBUTE	X-Ascend-FCP-Parameter			119	string
ATTRIBUTE	X-Ascend-Modem-PortNo			120	integer
ATTRIBUTE	X-Ascend-Modem-SlotNo			121	integer
ATTRIBUTE	X-Ascend-Modem-ShelfNo			122	integer
ATTRIBUTE	X-Ascend-Call-Attempt-Limit		123	integer
ATTRIBUTE	X-Ascend-Call-Block-Duration		124	integer
ATTRIBUTE	X-Ascend-Maximum-Call-Duration		125	integer
ATTRIBUTE	X-Ascend-Temporary-Rtes			126	integer
ATTRIBUTE       X-Ascend-Tunneling-Protocol             127     integer
ATTRIBUTE       X-Ascend-Shared-Profile-Enable    	128     integer
ATTRIBUTE	X-Ascend-Primary-Home-Agent		129	string
ATTRIBUTE	X-Ascend-Secondary-Home-Agent		130	string
ATTRIBUTE	X-Ascend-Dialout-Allowed		131	integer
ATTRIBUTE	X-Ascend-Client-Gateway			132	ipaddr
ATTRIBUTE	X-Ascend-BACP-Enable			133	integer
ATTRIBUTE	X-Ascend-DHCP-Maximum-Leases		134	integer
ATTRIBUTE	X-Ascend-Client-Primary-DNS		135	ipaddr
ATTRIBUTE	X-Ascend-Client-Secondary-DNS		136	ipaddr
ATTRIBUTE	X-Ascend-Client-Assign-DNS		137	integer
ATTRIBUTE	X-Ascend-User-Acct-Type			138	integer
ATTRIBUTE	X-Ascend-User-Acct-Host			139	ipaddr
ATTRIBUTE	X-Ascend-User-Acct-Port			140	integer
ATTRIBUTE	X-Ascend-User-Acct-Key			141	string
ATTRIBUTE	X-Ascend-User-Acct-Base			142	integer
ATTRIBUTE	X-Ascend-User-Acct-Time			143	integer
ATTRIBUTE	X-Ascend-Assign-IP-Client		144	ipaddr
ATTRIBUTE	X-Ascend-Assign-IP-Server		145	ipaddr
ATTRIBUTE	X-Ascend-Assign-IP-Global-Pool		146	string
ATTRIBUTE	X-Ascend-DHCP-Reply			147	integer
ATTRIBUTE	X-Ascend-DHCP-Pool-Number		148	integer
ATTRIBUTE	X-Ascend-Expect-Callback		149	integer
ATTRIBUTE	X-Ascend-Event-Type			150	integer
ATTRIBUTE	X-Ascend-Session-Svr-Key		151	string
ATTRIBUTE	X-Ascend-Multicast-Rate-Limit		152	integer
ATTRIBUTE	X-Ascend-IF-Netmask			153	ipaddr
ATTRIBUTE	X-Ascend-Remote-Addr			154	ipaddr
ATTRIBUTE	X-Ascend-Multicast-Client		155	integer
ATTRIBUTE	X-Ascend-FR-Circuit-Name		156	string
ATTRIBUTE	X-Ascend-FR-LinkUp			157	integer
ATTRIBUTE	X-Ascend-FR-Nailed-Grp			158	integer
ATTRIBUTE	X-Ascend-FR-Type			159	integer
ATTRIBUTE	X-Ascend-FR-Link-Mgt			160	integer
ATTRIBUTE	X-Ascend-FR-N391			161	integer
ATTRIBUTE	X-Ascend-FR-DCE-N392			162	integer
ATTRIBUTE	X-Ascend-FR-DTE-N392			163	integer
ATTRIBUTE	X-Ascend-FR-DCE-N393			164	integer
ATTRIBUTE	X-Ascend-FR-DTE-N393			165	integer
ATTRIBUTE	X-Ascend-FR-T391			166	integer
ATTRIBUTE	X-Ascend-FR-T392			167	integer
ATTRIBUTE	X-Ascend-Bridge-Address  	 	168	string
ATTRIBUTE       X-Ascend-TS-Idle-Limit            	169     integer
ATTRIBUTE       X-Ascend-TS-Idle-Mode             	170     integer
ATTRIBUTE	X-Ascend-DBA-Monitor	 		171	integer
ATTRIBUTE	X-Ascend-Base-Channel-Count 		172	integer
ATTRIBUTE	X-Ascend-Minimum-Channels		173	integer
ATTRIBUTE	X-Ascend-IPX-Route			174	string
ATTRIBUTE	X-Ascend-FT1-Caller			175	integer
ATTRIBUTE	X-Ascend-Backup				176	string
ATTRIBUTE	X-Ascend-Call-Type			177	integer
ATTRIBUTE	X-Ascend-Group				178	string
ATTRIBUTE	X-Ascend-FR-DLCI			179	integer
ATTRIBUTE	X-Ascend-FR-Profile-Name		180	string
ATTRIBUTE	X-Ascend-Ara-PW				181	string
ATTRIBUTE	X-Ascend-IPX-Node-Addr			182	string
ATTRIBUTE	X-Ascend-Home-Agent-IP-Addr		183	ipaddr
ATTRIBUTE	X-Ascend-Home-Agent-Password		184	string
ATTRIBUTE	X-Ascend-Home-Network-Name		185	string
ATTRIBUTE	X-Ascend-Home-Agent-UDP-Port		186	integer
ATTRIBUTE	X-Ascend-Multilink-ID			187	integer
ATTRIBUTE	X-Ascend-Num-In-Multilink		188	integer
ATTRIBUTE	X-Ascend-First-Dest			189	ipaddr
ATTRIBUTE	X-Ascend-Pre-Input-Octets		190	integer
ATTRIBUTE	X-Ascend-Pre-Output-Octets		191	integer
ATTRIBUTE	X-Ascend-Pre-Input-Packets		192	integer
ATTRIBUTE	X-Ascend-Pre-Output-Packets		193	integer
ATTRIBUTE	X-Ascend-Maximum-Time			194	integer
ATTRIBUTE	X-Ascend-Disconnect-Cause		195	integer
ATTRIBUTE	X-Ascend-Connect-Progress		196	integer
ATTRIBUTE	X-Ascend-Data-Rate			197	integer
ATTRIBUTE	X-Ascend-PreSession-Time		198	integer
ATTRIBUTE	X-Ascend-Token-Idle			199	integer
ATTRIBUTE	X-Ascend-Token-Immediate		200	integer
ATTRIBUTE	X-Ascend-Require-Auth			201	integer
ATTRIBUTE	X-Ascend-Number-Sessions		202	string
ATTRIBUTE	X-Ascend-Authen-Alias			203	string
ATTRIBUTE	X-Ascend-Token-Expiry			204	integer
ATTRIBUTE	X-Ascend-Menu-Selector			205	string
ATTRIBUTE	X-Ascend-Menu-Item			206	string
ATTRIBUTE	X-Ascend-PW-Warntime			207	integer
ATTRIBUTE	X-Ascend-PW-Lifetime			208	integer
ATTRIBUTE	X-Ascend-IP-Direct			209	ipaddr
ATTRIBUTE	X-Ascend-PPP-VJ-Slot-Comp		210	integer
ATTRIBUTE	X-Ascend-PPP-VJ-1172			211	integer
ATTRIBUTE	X-Ascend-PPP-Async-Map			212	integer
ATTRIBUTE	X-Ascend-Third-Prompt			213	string
ATTRIBUTE	X-Ascend-Send-Secret			214	string encrypt=3
ATTRIBUTE	X-Ascend-Receive-Secret			215	string encrypt=3
ATTRIBUTE	X-Ascend-IPX-Peer-Mode			216	integer
ATTRIBUTE	X-Ascend-IP-Pool-Definition		217	string
ATTRIBUTE	X-Ascend-Assign-IP-Pool			218	integer
ATTRIBUTE	X-Ascend-FR-Direct			219	integer
ATTRIBUTE	X-Ascend-FR-Direct-Profile		220	string
ATTRIBUTE	X-Ascend-FR-Direct-DLCI			221	integer
ATTRIBUTE	X-Ascend-Handle-IPX			222	integer
ATTRIBUTE	X-Ascend-Netware-timeout		223	integer
ATTRIBUTE	X-Ascend-IPX-Alias			224	integer
ATTRIBUTE	X-Ascend-Metric				225	integer
ATTRIBUTE	X-Ascend-PRI-Number-Type		226	integer
ATTRIBUTE	X-Ascend-Dial-Number			227	string
ATTRIBUTE	X-Ascend-Route-IP			228	integer
ATTRIBUTE	X-Ascend-Route-IPX			229	integer
ATTRIBUTE	X-Ascend-Bridge				230	integer
ATTRIBUTE	X-Ascend-Send-Auth			231	integer
ATTRIBUTE	X-Ascend-Send-Passwd			232	string
ATTRIBUTE	X-Ascend-Link-Compression		233	integer
ATTRIBUTE	X-Ascend-Target-Util			234	integer
ATTRIBUTE	X-Ascend-Maximum-Channels		235	integer
ATTRIBUTE	X-Ascend-Inc-Channel-Count		236	integer
ATTRIBUTE	X-Ascend-Dec-Channel-Count		237	integer
ATTRIBUTE	X-Ascend-Seconds-Of-History		238	integer
ATTRIBUTE	X-Ascend-History-Weigh-Type		239	integer
ATTRIBUTE	X-Ascend-Add-Seconds			240	integer
ATTRIBUTE	X-Ascend-Remove-Seconds			241	integer
ATTRIBUTE	X-Ascend-Data-Filter			242	string
ATTRIBUTE	X-Ascend-Call-Filter			243	string
ATTRIBUTE	X-Ascend-Idle-Limit			244	integer
ATTRIBUTE	X-Ascend-Preempt-Limit			245	integer
ATTRIBUTE	X-Ascend-Callback			246	integer
ATTRIBUTE	X-Ascend-Data-Svc			247	integer
ATTRIBUTE	X-Ascend-Force-56			248	integer
ATTRIBUTE	X-Ascend-Billing-Number			249	string
ATTRIBUTE	X-Ascend-Call-By-Call			250	integer
ATTRIBUTE	X-Ascend-Transit-Number			251	string
ATTRIBUTE	X-Ascend-Host-Info			252	string
ATTRIBUTE	X-Ascend-PPP-Address			253	ipaddr
ATTRIBUTE	X-Ascend-MPP-Idle-Percent		254	integer
ATTRIBUTE	X-Ascend-Xmit-Rate			255	integer

#
#  Ascend vendor-specific attributes.
#
BEGIN-VENDOR Ascend
ATTRIBUTE	Ascend-Max-Shared-Users		2	integer
ATTRIBUTE	Ascend-UU-Info			7	string
ATTRIBUTE	Ascend-CIR-Timer		9	integer
ATTRIBUTE	Ascend-FR-08-Mode		10	integer
ATTRIBUTE	Ascend-Destination-Nas-Port	11	integer
ATTRIBUTE	Ascend-FR-SVC-Addr		12	string
ATTRIBUTE	Ascend-NAS-Port-Format		13	integer
ATTRIBUTE	Ascend-ATM-Fault-Management	14	integer
ATTRIBUTE	Ascend-ATM-Loopback-Cell-Loss	15	integer
ATTRIBUTE	Ascend-Ckt-Type			16	integer
ATTRIBUTE	Ascend-SVC-Enabled		17	integer
ATTRIBUTE	Ascend-Session-Type		18	integer
ATTRIBUTE	Ascend-H323-Gatekeeper		19	ipaddr
ATTRIBUTE	Ascend-Global-Call-Id		20	string
ATTRIBUTE	Ascend-H323-Conference-Id	21	integer
ATTRIBUTE	Ascend-H323-Fegw-Address	22	ipaddr
ATTRIBUTE	Ascend-H323-Dialed-Time		23	integer
ATTRIBUTE	Ascend-Dialed-Number		24	string
ATTRIBUTE	Ascend-Inter-Arrival-Jitter	25	integer
ATTRIBUTE	Ascend-Dropped-Octets		26	integer
ATTRIBUTE	Ascend-Dropped-Packets		27	integer
ATTRIBUTE	Ascend-Auth-Delay		28	integer
ATTRIBUTE	Ascend-X25-Pad-X3-Profile	29	integer
ATTRIBUTE	Ascend-X25-Pad-X3-Parameters	30	string
ATTRIBUTE	Ascend-Tunnel-VRouter-Name	31	string
ATTRIBUTE	Ascend-X25-Reverse-Charging	32	integer
ATTRIBUTE	Ascend-X25-Nui-Prompt		33	string
ATTRIBUTE	Ascend-X25-Nui-Password-Prompt	34	string
ATTRIBUTE	Ascend-X25-Cug			35	string
ATTRIBUTE	Ascend-X25-Pad-Alias-1		36	string
ATTRIBUTE	Ascend-X25-Pad-Alias-2		37	string
ATTRIBUTE	Ascend-X25-Pad-Alias-3		38	string
ATTRIBUTE	Ascend-X25-X121-Address		39	string
ATTRIBUTE	Ascend-X25-Nui			40	string
ATTRIBUTE	Ascend-X25-Rpoa			41	string
ATTRIBUTE	Ascend-X25-Pad-Prompt		42	string
ATTRIBUTE	Ascend-X25-Pad-Banner		43	string
ATTRIBUTE	Ascend-X25-Profile-Name		44	string
ATTRIBUTE	Ascend-Recv-Name		45	string
ATTRIBUTE	Ascend-Bi-Directional-Auth	46	integer
ATTRIBUTE	Ascend-MTU			47	integer
ATTRIBUTE	Ascend-Call-Direction		48	integer
ATTRIBUTE	Ascend-Service-Type		49	integer
ATTRIBUTE	Ascend-Filter-Required		50	integer
ATTRIBUTE	Ascend-Traffic-Shaper		51	integer
ATTRIBUTE	Ascend-Access-Intercept-LEA	52	string
ATTRIBUTE	Ascend-Access-Intercept-Log	53	string
ATTRIBUTE	Ascend-Private-Route-Table-ID	54	string
ATTRIBUTE	Ascend-Private-Route-Required	55	integer
ATTRIBUTE	Ascend-Cache-Refresh		56	integer
ATTRIBUTE	Ascend-Cache-Time		57	integer
ATTRIBUTE	Ascend-Egress-Enabled		58	integer
ATTRIBUTE	Ascend-QOS-Upstream		59	string
ATTRIBUTE	Ascend-QOS-Downstream		60	string
ATTRIBUTE	Ascend-ATM-Connect-Vpi		61	integer
ATTRIBUTE	Ascend-ATM-Connect-Vci		62	integer
ATTRIBUTE	Ascend-ATM-Connect-Group	63	integer
ATTRIBUTE	Ascend-ATM-Group		64	integer
ATTRIBUTE	Ascend-IPX-Header-Compression	65	integer
ATTRIBUTE	Ascend-Calling-Id-Type-Of-Num	66	integer
ATTRIBUTE	Ascend-Calling-Id-Number-Plan	67	integer
ATTRIBUTE	Ascend-Calling-Id-Presentatn	68	integer
ATTRIBUTE	Ascend-Calling-Id-Screening	69	integer
ATTRIBUTE	Ascend-BIR-Enable		70	integer
ATTRIBUTE	Ascend-BIR-Proxy		71	integer
ATTRIBUTE	Ascend-BIR-Bridge-Group		72	integer
ATTRIBUTE	Ascend-IPSEC-Profile		73	string
ATTRIBUTE	Ascend-PPPoE-Enable		74	integer
ATTRIBUTE	Ascend-Bridge-Non-PPPoE		75	integer
ATTRIBUTE	Ascend-ATM-Direct		76	integer
ATTRIBUTE	Ascend-ATM-Direct-Profile	77	string
ATTRIBUTE	Ascend-Client-Primary-WINS	78	ipaddr
ATTRIBUTE	Ascend-Client-Secondary-WINS	79	ipaddr
ATTRIBUTE	Ascend-Client-Assign-WINS	80	integer
ATTRIBUTE	Ascend-Auth-Type		81	integer
ATTRIBUTE	Ascend-Port-Redir-Protocol	82	integer
ATTRIBUTE	Ascend-Port-Redir-Portnum	83	integer
ATTRIBUTE	Ascend-Port-Redir-Server	84	ipaddr
ATTRIBUTE	Ascend-IP-Pool-Chaining		85	integer
ATTRIBUTE	Ascend-Owner-IP-Addr		86	ipaddr
ATTRIBUTE	Ascend-IP-TOS			87	integer
ATTRIBUTE	Ascend-IP-TOS-Precedence	88	integer
ATTRIBUTE	Ascend-IP-TOS-Apply-To		89	integer
ATTRIBUTE	Ascend-Filter			90	string
ATTRIBUTE	Ascend-Telnet-Profile		91	string
ATTRIBUTE	Ascend-Dsl-Rate-Type		92	integer
ATTRIBUTE	Ascend-Redirect-Number		93	string
ATTRIBUTE	Ascend-ATM-Vpi			94	integer
ATTRIBUTE	Ascend-ATM-Vci			95	integer
ATTRIBUTE	Ascend-Source-IP-Check		96	integer
ATTRIBUTE	Ascend-Dsl-Rate-Mode		97	integer
ATTRIBUTE	Ascend-Dsl-Upstream-Limit	98	integer
ATTRIBUTE	Ascend-Dsl-Downstream-Limit	99	integer
ATTRIBUTE	Ascend-Dsl-CIR-Recv-Limit	100	integer
ATTRIBUTE	Ascend-Dsl-CIR-Xmit-Limit	101	integer
ATTRIBUTE	Ascend-VRouter-Name		102	string
ATTRIBUTE	Ascend-Source-Auth		103	string
ATTRIBUTE	Ascend-Private-Route		104	string
ATTRIBUTE	Ascend-Numbering-Plan-ID	105	integer
ATTRIBUTE	Ascend-FR-Link-Status-DLCI	106	integer
ATTRIBUTE	Ascend-Calling-Subaddress	107	string
ATTRIBUTE	Ascend-Callback-Delay		108	integer
ATTRIBUTE	Ascend-Endpoint-Disc		109	string
ATTRIBUTE	Ascend-Remote-FW		110	string
ATTRIBUTE	Ascend-Multicast-GLeave-Delay	111	integer
ATTRIBUTE	Ascend-CBCP-Enable		112	integer
ATTRIBUTE	Ascend-CBCP-Mode		113	integer
ATTRIBUTE	Ascend-CBCP-Delay		114	integer
ATTRIBUTE	Ascend-CBCP-Trunk-Group		115	integer
ATTRIBUTE	Ascend-Appletalk-Route		116	string
ATTRIBUTE	Ascend-Appletalk-Peer-Mode	117	integer
ATTRIBUTE	Ascend-Route-Appletalk		118	integer
ATTRIBUTE	Ascend-FCP-Parameter		119	string
ATTRIBUTE	Ascend-Modem-PortNo		120	integer
ATTRIBUTE	Ascend-Modem-SlotNo		121	integer
ATTRIBUTE	Ascend-Modem-ShelfNo		122	integer
ATTRIBUTE	Ascend-Call-Attempt-Limit	123	integer
ATTRIBUTE	Ascend-Call-Block-Duration	124	integer
ATTRIBUTE	Ascend-Maximum-Call-Duration	125	integer
ATTRIBUTE	Ascend-Temporary-Rtes		126	integer
ATTRIBUTE       Ascend-Tunneling-Protocol       127     integer
ATTRIBUTE       Ascend-Shared-Profile-Enable    128     integer
ATTRIBUTE	Ascend-Primary-Home-Agent	129	string
ATTRIBUTE	Ascend-Secondary-Home-Agent	130	string
ATTRIBUTE	Ascend-Dialout-Allowed		131	integer
ATTRIBUTE	Ascend-Client-Gateway		132	ipaddr
ATTRIBUTE	Ascend-BACP-Enable		133	integer
ATTRIBUTE	Ascend-DHCP-Maximum-Leases	134	integer
ATTRIBUTE	Ascend-Client-Primary-DNS	135	ipaddr
ATTRIBUTE	Ascend-Client-Secondary-DNS	136	ipaddr
ATTRIBUTE	Ascend-Client-Assign-DNS	137	integer
ATTRIBUTE	Ascend-User-Acct-Type		138	integer
ATTRIBUTE	Ascend-User-Acct-Host		139	ipaddr
ATTRIBUTE	Ascend-User-Acct-Port		140	integer
ATTRIBUTE	Ascend-User-Acct-Key		141	string
ATTRIBUTE	Ascend-User-Acct-Base		142	integer
ATTRIBUTE	Ascend-User-Acct-Time		143	integer
ATTRIBUTE	Ascend-Assign-IP-Client		144	ipaddr
ATTRIBUTE	Ascend-Assign-IP-Server		145	ipaddr
ATTRIBUTE	Ascend-Assign-IP-Global-Pool	146	string
ATTRIBUTE	Ascend-DHCP-Reply		147	integer
ATTRIBUTE	Ascend-DHCP-Pool-Number		148	integer
ATTRIBUTE	Ascend-Expect-Callback		149	integer
ATTRIBUTE	Ascend-Event-Type		150	integer
ATTRIBUTE	Ascend-Session-Svr-Key		151	string
ATTRIBUTE	Ascend-Multicast-Rate-Limit	152	integer
ATTRIBUTE	Ascend-IF-Netmask		153	ipaddr
ATTRIBUTE	Ascend-Remote-Addr		154	ipaddr
ATTRIBUTE	Ascend-Multicast-Client		155	integer
ATTRIBUTE	Ascend-FR-Circuit-Name		156	string
ATTRIBUTE	Ascend-FR-LinkUp		157	integer
ATTRIBUTE	Ascend-FR-Nailed-Grp		158	integer
ATTRIBUTE	Ascend-FR-Type			159	integer
ATTRIBUTE	Ascend-FR-Link-Mgt		160	integer
ATTRIBUTE	Ascend-FR-N391			161	integer
ATTRIBUTE	Ascend-FR-DCE-N392		162	integer
ATTRIBUTE	Ascend-FR-DTE-N392		163	integer
ATTRIBUTE	Ascend-FR-DCE-N393		164	integer
ATTRIBUTE	Ascend-FR-DTE-N393		165	integer
ATTRIBUTE	Ascend-FR-T391			166	integer
ATTRIBUTE	Ascend-FR-T392			167	integer
ATTRIBUTE	Ascend-Bridge-Address  	 	168	string
ATTRIBUTE       Ascend-TS-Idle-Limit            169     integer
ATTRIBUTE       Ascend-TS-Idle-Mode             170     integer
ATTRIBUTE	Ascend-DBA-Monitor	 	171	integer
ATTRIBUTE	Ascend-Base-Channel-Count 	172	integer
ATTRIBUTE	Ascend-Minimum-Channels		173	integer
ATTRIBUTE	Ascend-IPX-Route		174	string
ATTRIBUTE	Ascend-FT1-Caller		175	integer
ATTRIBUTE	Ascend-Backup			176	string
ATTRIBUTE	Ascend-Call-Type		177	integer
ATTRIBUTE	Ascend-Group			178	string
ATTRIBUTE	Ascend-FR-DLCI			179	integer
ATTRIBUTE	Ascend-FR-Profile-Name		180	string
ATTRIBUTE	Ascend-Ara-PW			181	string
ATTRIBUTE	Ascend-IPX-Node-Addr		182	string
ATTRIBUTE	Ascend-Home-Agent-IP-Addr	183	ipaddr
ATTRIBUTE	Ascend-Home-Agent-Password	184	string
ATTRIBUTE	Ascend-Home-Network-Name	185	string
ATTRIBUTE	Ascend-Home-Agent-UDP-Port	186	integer
ATTRIBUTE	Ascend-Multilink-ID		187	integer
ATTRIBUTE	Ascend-Num-In-Multilink		188	integer
ATTRIBUTE	Ascend-First-Dest		189	ipaddr
ATTRIBUTE	Ascend-Pre-Input-Octets		190	integer
ATTRIBUTE	Ascend-Pre-Output-Octets	191	integer
ATTRIBUTE	Ascend-Pre-Input-Packets	192	integer
ATTRIBUTE	Ascend-Pre-Output-Packets	193	integer
ATTRIBUTE	Ascend-Maximum-Time		194	integer
ATTRIBUTE	Ascend-Disconnect-Cause		195	integer
ATTRIBUTE	Ascend-Connect-Progress		196	integer
ATTRIBUTE	Ascend-Data-Rate		197	integer
ATTRIBUTE	Ascend-PreSession-Time		198	integer
ATTRIBUTE	Ascend-Token-Idle		199	integer
ATTRIBUTE	Ascend-Token-Immediate		200	integer
ATTRIBUTE	Ascend-Require-Auth		201	integer
ATTRIBUTE	Ascend-Number-Sessions		202	string
ATTRIBUTE	Ascend-Authen-Alias		203	string
ATTRIBUTE	Ascend-Token-Expiry		204	integer
ATTRIBUTE	Ascend-Menu-Selector		205	string
ATTRIBUTE	Ascend-Menu-Item		206	string
ATTRIBUTE	Ascend-PW-Warntime		207	integer
ATTRIBUTE	Ascend-PW-Lifetime		208	integer
ATTRIBUTE	Ascend-IP-Direct		209	ipaddr
ATTRIBUTE	Ascend-PPP-VJ-Slot-Comp		210	integer
ATTRIBUTE	Ascend-PPP-VJ-1172		211	integer
ATTRIBUTE	Ascend-PPP-Async-Map		212	integer
ATTRIBUTE	Ascend-Third-Prompt		213	string
ATTRIBUTE	Ascend-Send-Secret		214	string	encrypt=3
ATTRIBUTE	Ascend-Receive-Secret		215	string	encrypt=3
ATTRIBUTE	Ascend-IPX-Peer-Mode		216	integer
ATTRIBUTE	Ascend-IP-Pool-Definition	217	string
ATTRIBUTE	Ascend-Assign-IP-Pool		218	integer
ATTRIBUTE	Ascend-FR-Direct		219	integer
ATTRIBUTE	Ascend-FR-Direct-Profile	220	string
ATTRIBUTE	Ascend-FR-Direct-DLCI		221	integer
ATTRIBUTE	Ascend-Handle-IPX		222	integer
ATTRIBUTE	Ascend-Netware-timeout		223	integer
ATTRIBUTE	Ascend-IPX-Alias		224	integer
ATTRIBUTE	Ascend-Metric			225	integer
ATTRIBUTE	Ascend-PRI-Number-Type		226	integer
ATTRIBUTE	Ascend-Dial-Number		227	string
ATTRIBUTE	Ascend-Route-IP			228	integer
ATTRIBUTE	Ascend-Route-IPX		229	integer
ATTRIBUTE	Ascend-Bridge			230	integer
ATTRIBUTE	Ascend-Send-Auth		231	integer
ATTRIBUTE	Ascend-Send-Passwd		232	string
ATTRIBUTE	Ascend-Link-Compression		233	integer
ATTRIBUTE	Ascend-Target-Util		234	integer
ATTRIBUTE	Ascend-Maximum-Channels		235	integer
ATTRIBUTE	Ascend-Inc-Channel-Count	236	integer
ATTRIBUTE	Ascend-Dec-Channel-Count	237	integer
ATTRIBUTE	Ascend-Seconds-Of-History	238	integer
ATTRIBUTE	Ascend-History-Weigh-Type	239	integer
ATTRIBUTE	Ascend-Add-Seconds		240	integer
ATTRIBUTE	Ascend-Remove-Seconds		241	integer
ATTRIBUTE	Ascend-Data-Filter		242	string
ATTRIBUTE	Ascend-Call-Filter		243	string
ATTRIBUTE	Ascend-Idle-Limit		244	integer
ATTRIBUTE	Ascend-Preempt-Limit		245	integer
ATTRIBUTE	Ascend-Callback			246	integer
ATTRIBUTE	Ascend-Data-Svc			247	integer
ATTRIBUTE	Ascend-Force-56			248	integer
ATTRIBUTE	Ascend-Billing-Number		249	string
ATTRIBUTE	Ascend-Call-By-Call		250	integer
ATTRIBUTE	Ascend-Transit-Number		251	string
ATTRIBUTE	Ascend-Host-Info		252	string
ATTRIBUTE	Ascend-PPP-Address		253	ipaddr
ATTRIBUTE	Ascend-MPP-Idle-Percent		254	integer
ATTRIBUTE	Ascend-Xmit-Rate		255	integer


# Ascend protocols
VALUE		Service-Type		Dialout-Framed-User	5
VALUE		Framed-Protocol		Ascend-ARA		255
VALUE		Framed-Protocol		Ascend-MPP		256
VALUE		Framed-Protocol		Ascend-EURAW		257
VALUE		Framed-Protocol		Ascend-EUUI		258
VALUE		Framed-Protocol		Ascend-X25		259
VALUE		Framed-Protocol		Ascend-COMB		260
VALUE		Framed-Protocol		Ascend-FR		261
VALUE		Framed-Protocol		Ascend-MP		262
VALUE		Framed-Protocol		Ascend-FR-CIR		263


#
#	Ascend specific extensions
#	Used by ASCEND MAX/Pipeline products (see above)
#

VALUE		Ascend-Source-IP-Check	Source-IP-Check-No	0
VALUE		Ascend-Source-IP-Check	Source-IP-Check-Yes	1
VALUE		Ascend-CBCP-Enable	CBCP-Not-Enabled	0
VALUE		Ascend-CBCP-Enable	CBCP-Enabled		1
VALUE		Ascend-CBCP-Mode	CBCP-No-Callback	1
VALUE		Ascend-CBCP-Mode	CBCP-User-Callback	2
VALUE		Ascend-CBCP-Mode	CBCP-Profile-Callback	3
VALUE		Ascend-CBCP-Mode	CBCP-Any-Or-No		7
VALUE		Ascend-CBCP-Mode	CBCP-Off		8
VALUE		Ascend-FR-Direct	FR-Direct-No		0
VALUE		Ascend-FR-Direct	FR-Direct-Yes		1
VALUE		Ascend-Handle-IPX	Handle-IPX-None		0
VALUE		Ascend-Handle-IPX	Handle-IPX-Client	1
VALUE		Ascend-Handle-IPX	Handle-IPX-Server	2
VALUE		Ascend-IPX-Peer-Mode	IPX-Peer-Router		0
VALUE		Ascend-IPX-Peer-Mode	IPX-Peer-Dialin		1
VALUE		Ascend-Call-Type	Switched		0
VALUE		Ascend-Call-Type	Nailed			1
VALUE		Ascend-Call-Type	Nailed/Mpp		2
VALUE		Ascend-Call-Type	Perm/Switched		3
VALUE		Ascend-Call-Type	AO/DI			6
VALUE		Ascend-Call-Type	MegaMax			7
VALUE		Ascend-FT1-Caller	FT1-No			0
VALUE		Ascend-FT1-Caller	FT1-Yes			1
VALUE		Ascend-PRI-Number-Type	Unknown-Number		0
VALUE		Ascend-PRI-Number-Type	Intl-Number		1
VALUE		Ascend-PRI-Number-Type	National-Number		2
VALUE		Ascend-PRI-Number-Type	Net-Specific-Number	3
VALUE		Ascend-PRI-Number-Type	Local-Number		4
VALUE		Ascend-PRI-Number-Type	Abbrev-Number		5

VALUE		Ascend-Route-IP		Route-IP-No		0
VALUE		Ascend-Route-IP		Route-IP-Yes		1
VALUE		Ascend-Route-IPX	Route-IPX-No		0
VALUE		Ascend-Route-IPX	Route-IPX-Yes		1
VALUE		Ascend-Bridge		Bridge-No		0
VALUE		Ascend-Bridge		Bridge-Yes		1
VALUE  		Ascend-TS-Idle-Mode     TS-Idle-None		0
VALUE	  	Ascend-TS-Idle-Mode     TS-Idle-Input		1
VALUE  		Ascend-TS-Idle-Mode     TS-Idle-Input-Output	2
VALUE		Ascend-Send-Auth	Send-Auth-None		0
VALUE		Ascend-Send-Auth	Send-Auth-PAP		1
VALUE		Ascend-Send-Auth	Send-Auth-CHAP		2
VALUE		Ascend-Send-Auth	Send-Auth-MS-CHAP	3
VALUE		Ascend-Link-Compression	Link-Comp-None		0
VALUE		Ascend-Link-Compression	Link-Comp-Stac		1
VALUE		Ascend-Link-Compression	Link-Comp-Stac-Draft-9	2
VALUE		Ascend-Link-Compression	Link-Comp-MS-Stac	3
VALUE		Ascend-History-Weigh-Type	History-Constant	0
VALUE		Ascend-History-Weigh-Type	History-Linear		1
VALUE		Ascend-History-Weigh-Type	History-Quadratic	2
VALUE		Ascend-Callback		Callback-No		0
VALUE		Ascend-Callback		Callback-Yes		1
VALUE		Ascend-Expect-Callback	Expect-Callback-No	0
VALUE		Ascend-Expect-Callback	Expect-Callback-Yes	1
VALUE		Ascend-Data-Svc		Switched-Voice-Bearer	0
VALUE		Ascend-Data-Svc		Nailed-56KR		1
VALUE		Ascend-Data-Svc		Nailed-64K		2
VALUE		Ascend-Data-Svc		Switched-64KR		3
VALUE		Ascend-Data-Svc		Switched-56K		4
VALUE		Ascend-Data-Svc		Switched-384KR		5
VALUE		Ascend-Data-Svc		Switched-384K		6
VALUE		Ascend-Data-Svc		Switched-1536K		7
VALUE		Ascend-Data-Svc		Switched-1536KR		8
VALUE		Ascend-Data-Svc		Switched-128K		9
VALUE		Ascend-Data-Svc		Switched-192K		10
VALUE		Ascend-Data-Svc		Switched-256K		11
VALUE		Ascend-Data-Svc		Switched-320K		12
VALUE		Ascend-Data-Svc		Switched-384K-MR	13
VALUE		Ascend-Data-Svc		Switched-448K		14
VALUE		Ascend-Data-Svc		Switched-512K		15
VALUE		Ascend-Data-Svc		Switched-576K		16
VALUE		Ascend-Data-Svc		Switched-640K		17
VALUE		Ascend-Data-Svc		Switched-704K		18
VALUE		Ascend-Data-Svc		Switched-768K		19
VALUE		Ascend-Data-Svc		Switched-832K		20
VALUE		Ascend-Data-Svc		Switched-896K		21
VALUE		Ascend-Data-Svc		Switched-960K		22
VALUE		Ascend-Data-Svc		Switched-1024K		23
VALUE		Ascend-Data-Svc		Switched-1088K		24
VALUE		Ascend-Data-Svc		Switched-1152K		25
VALUE		Ascend-Data-Svc		Switched-1216K		26
VALUE		Ascend-Data-Svc		Switched-1280K		27
VALUE		Ascend-Data-Svc		Switched-1344K		28
VALUE		Ascend-Data-Svc		Switched-1408K		29
VALUE		Ascend-Data-Svc		Switched-1472K		30
VALUE		Ascend-Data-Svc		Switched-1600K		31
VALUE		Ascend-Data-Svc		Switched-1664K		32
VALUE		Ascend-Data-Svc		Switched-1728K		33
VALUE		Ascend-Data-Svc		Switched-1792K		34
VALUE		Ascend-Data-Svc		Switched-1856K		35
VALUE		Ascend-Data-Svc		Switched-1920K		36
VALUE		Ascend-Data-Svc		Switched-inherited		37
VALUE		Ascend-Data-Svc		Switched-restricted-bearer-x30  38
VALUE		Ascend-Data-Svc		Switched-clear-bearer-v110	39
VALUE		Ascend-Data-Svc		Switched-restricted-64-x30	40
VALUE		Ascend-Data-Svc		Switched-clear-56-v110		41
VALUE		Ascend-Data-Svc		Switched-modem			42
VALUE		Ascend-Data-Svc		Switched-atmodem		43
VALUE		Ascend-Data-Svc		Switched-V110-24-56	45
VALUE		Ascend-Data-Svc		Switched-V110-48-56	46
VALUE		Ascend-Data-Svc		Switched-V110-96-56	47
VALUE		Ascend-Data-Svc		Switched-V110-192-56	48
VALUE		Ascend-Data-Svc		Switched-V110-384-56	49
VALUE		Ascend-Data-Svc		Switched-V110-24-56R	50
VALUE		Ascend-Data-Svc		Switched-V110-48-56R	51
VALUE		Ascend-Data-Svc		Switched-V110-96-56R	52
VALUE		Ascend-Data-Svc		Switched-V110-192-56R	53
VALUE		Ascend-Data-Svc		Switched-V110-384-56R	54
VALUE		Ascend-Data-Svc		Switched-V110-24-64	55
VALUE		Ascend-Data-Svc		Switched-V110-48-64	56
VALUE		Ascend-Data-Svc		Switched-V110-96-64	57
VALUE		Ascend-Data-Svc		Switched-V110-192-64	58
VALUE		Ascend-Data-Svc		Switched-V110-384-64	59
VALUE		Ascend-Data-Svc		Switched-V110-24-64R	60
VALUE		Ascend-Data-Svc		Switched-V110-48-64R	61
VALUE		Ascend-Data-Svc		Switched-V110-96-64R	62
VALUE		Ascend-Data-Svc		Switched-V110-384-64R	64
VALUE		Ascend-Data-Svc		Switched-V110-192-64R	63

VALUE		Ascend-Data-Svc		Switched-Pots		68
VALUE		Ascend-Data-Svc		Switched-ATM		69
VALUE		Ascend-Data-Svc		Switched-FR		70

VALUE		Ascend-Force-56		Force-56-No		0
VALUE		Ascend-Force-56		Force-56-Yes		1
VALUE		Ascend-PW-Lifetime	Lifetime-In-Days	0
VALUE		Ascend-PW-Warntime	Days-Of-Warning		0
VALUE		Ascend-PPP-VJ-1172	PPP-VJ-1172		1
VALUE		Ascend-PPP-VJ-Slot-Comp	VJ-Slot-Comp-No		1
VALUE		Ascend-Require-Auth	Not-Require-Auth	0
VALUE		Ascend-Require-Auth	Require-Auth		1
VALUE		Ascend-Token-Immediate	Tok-Imm-No		0
VALUE		Ascend-Token-Immediate	Tok-Imm-Yes		1
VALUE		Ascend-DBA-Monitor	DBA-Transmit		0
VALUE 		Ascend-DBA-Monitor	DBA-Transmit-Recv	1
VALUE		Ascend-DBA-Monitor	DBA-None		2
VALUE		Ascend-FR-Type		Ascend-FR-DTE		0
VALUE		Ascend-FR-Type		Ascend-FR-DCE		1
VALUE		Ascend-FR-Type		Ascend-FR-NNI		2
VALUE		Ascend-FR-Link-Mgt	Ascend-FR-No-Link-Mgt	0
VALUE		Ascend-FR-Link-Mgt	Ascend-FR-T1-617D	1
VALUE		Ascend-FR-Link-Mgt	Ascend-FR-Q-933A	2
VALUE		Ascend-FR-LinkUp	Ascend-LinkUp-Default	0
VALUE		Ascend-FR-LinkUp	Ascend-LinkUp-AlwaysUp	1
VALUE		Ascend-Multicast-Client	Multicast-No		0
VALUE		Ascend-Multicast-Client	Multicast-Yes		1
VALUE		Ascend-User-Acct-Type	Ascend-User-Acct-None	0
VALUE		Ascend-User-Acct-Type	Ascend-User-Acct-User	1
VALUE		Ascend-User-Acct-Type	Ascend-User-Acct-User-Default	2
VALUE		Ascend-User-Acct-Base	Base-10			0
VALUE		Ascend-User-Acct-Base	Base-16			1
VALUE		Ascend-DHCP-Reply	DHCP-Reply-No		0
VALUE		Ascend-DHCP-Reply	DHCP-Reply-Yes		1
VALUE		Ascend-Client-Assign-DNS	DNS-Assign-No		0
VALUE		Ascend-Client-Assign-DNS	DNS-Assign-Yes		1
VALUE		Ascend-Event-Type	Ascend-ColdStart	1
VALUE		Ascend-Event-Type	Ascend-Session-Event	2
VALUE		Ascend-BACP-Enable	BACP-No			0
VALUE		Ascend-BACP-Enable	BACP-Yes		1
VALUE		Ascend-Dialout-Allowed	Dialout-Not-Allowed	0
VALUE		Ascend-Dialout-Allowed	Dialout-Allowed		1
VALUE		Ascend-Shared-Profile-Enable    Shared-Profile-No       0
VALUE		Ascend-Shared-Profile-Enable    Shared-Profile-Yes      1
VALUE		Ascend-Temporary-Rtes	Temp-Rtes-No		0
VALUE		Ascend-Temporary-Rtes	Temp-Rtes-Yes		1

# Ascend Disconnect Cause Values

VALUE		Ascend-Disconnect-Cause No-Reason			0
VALUE		Ascend-Disconnect-Cause Not-Applicable			1
VALUE		Ascend-Disconnect-Cause Unknown				2
VALUE		Ascend-Disconnect-Cause Call-Disconnected		3
VALUE		Ascend-Disconnect-Cause CLID-Authentication-Failed	4
VALUE		Ascend-Disconnect-Cause CLID-RADIUS-Timeout		5

VALUE		Ascend-Disconnect-Cause Modem-No-DCD			10
VALUE		Ascend-Disconnect-Cause DCD-Detected-Then-Inactive	11
VALUE		Ascend-Disconnect-Cause Modem-Invalid-Result-Codes	12

VALUE		Ascend-Disconnect-Cause TermSrv-User-Quit		20
VALUE		Ascend-Disconnect-Cause TermSrv-Idle-Timeout		21
VALUE		Ascend-Disconnect-Cause TermSrv-Exit-Telnet		22
VALUE		Ascend-Disconnect-Cause TermSrv-No-IPaddr		23
VALUE		Ascend-Disconnect-Cause TermSrv-Exit-Raw-TCP		24
VALUE		Ascend-Disconnect-Cause TermSrv-Exit-Login-Failed	25
VALUE		Ascend-Disconnect-Cause TermSrv-Exit-Raw-TCP-Disabled	26
VALUE		Ascend-Disconnect-Cause TermSrv-CTRL-C-In-Login		27
VALUE		Ascend-Disconnect-Cause TermSrv-Destroyed		28
VALUE		Ascend-Disconnect-Cause TermSrv-User-Closed-VCon	29

VALUE		Ascend-Disconnect-Cause TermSrv-VCon-Destroyed		30
VALUE		Ascend-Disconnect-Cause TermSrv-Exit-Rlogin		31
VALUE		Ascend-Disconnect-Cause TermSrv-Bad-Rlogin-Option	32
VALUE		Ascend-Disconnect-Cause TermSrv-Not-Enough-Resources	33

VALUE		Ascend-Disconnect-Cause MPP-No-NULL-Msg-Timeout		35

VALUE		Ascend-Disconnect-Cause PPP-LCP-Timeout			40
VALUE		Ascend-Disconnect-Cause PPP-LCP-Negotion-Failed		41
VALUE		Ascend-Disconnect-Cause PPP-PAP-Auth-Failed		42
VALUE		Ascend-Disconnect-Cause PPP-CHAP-Auth-Failed		43
VALUE		Ascend-Disconnect-Cause PPP-Rmt-Auth-Failed		44
VALUE		Ascend-Disconnect-Cause PPP-Rcv-Terminate-Req		45
VALUE		Ascend-Disconnect-Cause PPP-Rcv-Close-Event		46
VALUE		Ascend-Disconnect-Cause PPP-No-NCPs-Open		47
VALUE		Ascend-Disconnect-Cause PPP-MP-Bundle-Unknown		48
VALUE		Ascend-Disconnect-Cause PPP-LCP-Close-MP-Add-Fail	49

VALUE		Ascend-Disconnect-Cause Session-Table-Full		50
VALUE		Ascend-Disconnect-Cause Out-Of-Resources		51
VALUE		Ascend-Disconnect-Cause Invalid-IP-Address		52
VALUE		Ascend-Disconnect-Cause Hostname-Resolution-Failed	53
VALUE		Ascend-Disconnect-Cause Bad-Or-Missing-Port-Number	54

VALUE		Ascend-Disconnect-Cause Host-Reset			60
VALUE		Ascend-Disconnect-Cause Connection-Refused		61
VALUE		Ascend-Disconnect-Cause Connection-Timeout		62
VALUE		Ascend-Disconnect-Cause Connection-Closed		63
VALUE		Ascend-Disconnect-Cause Network-Unreachable		64
VALUE		Ascend-Disconnect-Cause Host-Unreachable		65
VALUE		Ascend-Disconnect-Cause Network-Unreachable-Admin	66
VALUE		Ascend-Disconnect-Cause Host-Unreachable-Admin		67
VALUE		Ascend-Disconnect-Cause Port-Unreachable		68

VALUE		Ascend-Disconnect-Cause Session-Timeout			100
VALUE		Ascend-Disconnect-Cause Invalid-Incoming-User		101
VALUE		Ascend-Disconnect-Cause Disconnect-Due-To-Callback	102

VALUE		Ascend-Disconnect-Cause Proto-Disabled-Or-Unsupported 120

VALUE		Ascend-Disconnect-Cause Disconnect-Req-By-RADIUS	150
VALUE		Ascend-Disconnect-Cause Disconnect-Req-By-Local-Admin	151

VALUE		Ascend-Disconnect-Cause V110-Timeout-Sync-Retry-Exceed 160

VALUE		Ascend-Disconnect-Cause PPP-Auth-Timeout-Exceeded	170
VALUE		Ascend-Disconnect-Cause User-Executed-Do-Hangup		180
VALUE		Ascend-Disconnect-Cause Remote-End-Hung-Up		185
VALUE		Ascend-Disconnect-Cause Resource-Has-Been-Quiesced	190
VALUE		Ascend-Disconnect-Cause Max-Call-Duration-Reached	195

# ascend connect progress codes
VALUE  Ascend-Connect-Progress No-Progress                     0
VALUE  Ascend-Connect-Progress Call-Up                         10
VALUE  Ascend-Connect-Progress Modem-Up                        30
VALUE  Ascend-Connect-Progress Modem-Awaiting-DCD              31
VALUE  Ascend-Connect-Progress Modem-Awaiting-Codes            32
VALUE  Ascend-Connect-Progress TermSrv-Started                 40
VALUE  Ascend-Connect-Progress TermSrv-Raw-TCP-Started         41
VALUE  Ascend-Connect-Progress TermSrv-Telnet-Started          42
VALUE  Ascend-Connect-Progress TermSrv-Raw-TCP-Connected       43
VALUE  Ascend-Connect-Progress TermSrv-Telnet-Connected        44
VALUE  Ascend-Connect-Progress TermSrv-Rlogin-Started          45
VALUE  Ascend-Connect-Progress TermSrv-Rlogin-Connected        46
VALUE  Ascend-Connect-Progress Modem-Outdial-Call-Up           50
VALUE  Ascend-Connect-Progress LAN-Session-Up                  60
VALUE  Ascend-Connect-Progress LCP-Opening                     61
VALUE  Ascend-Connect-Progress CCP-Opening                     62
VALUE  Ascend-Connect-Progress IPNCP-Opening                   63
VALUE  Ascend-Connect-Progress BNCP-Opening                    64
VALUE  Ascend-Connect-Progress LCP-Opened                      65
VALUE  Ascend-Connect-Progress CCP-Opened                      66
VALUE  Ascend-Connect-Progress IPNCP-Opened                    67
VALUE  Ascend-Connect-Progress BNCP-Opened                     68
VALUE  Ascend-Connect-Progress LCP-State-Initial               69
VALUE  Ascend-Connect-Progress LCP-State-Starting              70
VALUE  Ascend-Connect-Progress LCP-State-Closed                71
VALUE  Ascend-Connect-Progress LCP-State-Stopped               72
VALUE  Ascend-Connect-Progress LCP-State-Closing               73
VALUE  Ascend-Connect-Progress LCP-State-Stopping              74
VALUE  Ascend-Connect-Progress LCP-State-Request-Sent          75
VALUE  Ascend-Connect-Progress LCP-State-Ack-Received          76
VALUE  Ascend-Connect-Progress LCP-State-Ack-Sent              77
VALUE  Ascend-Connect-Progress IPXNCP-Opened                   80
VALUE  Ascend-Connect-Progress ATNCP-Opened                    81
VALUE  Ascend-Connect-Progress BACP-Opening                    82
VALUE  Ascend-Connect-Progress BACP-Opened                     83
VALUE  Ascend-Connect-Progress V110-Up                         90
VALUE  Ascend-Connect-Progress V110-State-Opened               91
VALUE  Ascend-Connect-Progress V110-State-Carrier              92
VALUE  Ascend-Connect-Progress V110-State-Reset                93
VALUE  Ascend-Connect-Progress V110-State-Closed               94
VALUE	Ascend-ATM-Direct		ATM-Direct-No	0
VALUE	Ascend-ATM-Direct		ATM-Direct-Yes	1
VALUE	Ascend-ATM-Fault-Management		VC-End-To-End-Loopback	2
VALUE	Ascend-ATM-Fault-Management		VC-No-Loopback	0
VALUE	Ascend-ATM-Fault-Management		VC-Segment-Loopback	1
VALUE	Ascend-Appletalk-Peer-Mode		Appletalk-Peer-Dialin	1
VALUE	Ascend-Appletalk-Peer-Mode		Appletalk-Peer-Router	0
VALUE	Ascend-Auth-Type		Auth-Any	2
VALUE	Ascend-Auth-Type		Auth-CHAP	4
VALUE	Ascend-Auth-Type		Auth-Default	1
VALUE	Ascend-Auth-Type		Auth-MS-CHAP	5
VALUE	Ascend-Auth-Type		Auth-None	0
VALUE	Ascend-Auth-Type		Auth-PAP	3
VALUE	Ascend-BIR-Enable		BIR-Enable-No	0
VALUE	Ascend-BIR-Enable		BIR-Enable-Yes	1
VALUE	Ascend-BIR-Proxy		BIR-Proxy-No	0
VALUE	Ascend-BIR-Proxy		BIR-Proxy-Yes	1
VALUE	Ascend-Bi-Directional-Auth		Bi-Directional-Auth-Allowed	1
VALUE	Ascend-Bi-Directional-Auth		Bi-Directional-Auth-None	0
VALUE	Ascend-Bi-Directional-Auth		Bi-Directional-Auth-Required	2
VALUE	Ascend-Bridge-Non-PPPoE		Bridge-Non-PPPoE-No	0
VALUE	Ascend-Bridge-Non-PPPoE		Bridge-Non-PPPoE-Yes	1
VALUE	Ascend-Cache-Refresh		Refresh-No	0
VALUE	Ascend-Cache-Refresh		Refresh-Yes	1
VALUE	Ascend-Call-Direction		Ascend-Call-Direction-Incoming	0
VALUE	Ascend-Call-Direction		Ascend-Call-Direction-Outgoing	1
VALUE	Ascend-Calling-Id-Number-Plan		Data	3
VALUE	Ascend-Calling-Id-Number-Plan		ISDN-Telephony	1
VALUE	Ascend-Calling-Id-Number-Plan		National	8
VALUE	Ascend-Calling-Id-Number-Plan		Private	9
VALUE	Ascend-Calling-Id-Number-Plan		Telex	4
VALUE	Ascend-Calling-Id-Number-Plan		Unknown	0
VALUE	Ascend-Calling-Id-Presentatn		Allowed	0
VALUE	Ascend-Calling-Id-Presentatn		Number-Not-Available	2
VALUE	Ascend-Calling-Id-Presentatn		Restricted	1
VALUE	Ascend-Calling-Id-Screening		Network-Provided	3
VALUE	Ascend-Calling-Id-Screening		User-Not-Screened	0
VALUE	Ascend-Calling-Id-Screening		User-Provided-Failed	2
VALUE	Ascend-Calling-Id-Screening		User-Provided-Passed	1
VALUE	Ascend-Calling-Id-Type-Of-Num		Abbreviated-Number	6
VALUE	Ascend-Calling-Id-Type-Of-Num		International-Number	1
VALUE	Ascend-Calling-Id-Type-Of-Num		National-Number	2
VALUE	Ascend-Calling-Id-Type-Of-Num		Network-Specific	3
VALUE	Ascend-Calling-Id-Type-Of-Num		Subscriber-Number	4
VALUE	Ascend-Calling-Id-Type-Of-Num		Unknown	0
VALUE	Ascend-Ckt-Type		Ascend-PVC	0
VALUE	Ascend-Ckt-Type		Ascend-SVC	1
VALUE	Ascend-Client-Assign-WINS		WINS-Assign-No	0
VALUE	Ascend-Client-Assign-WINS		WINS-Assign-Yes	1

VALUE	Ascend-Dsl-Downstream-Limit		adslcap-dn-1280000	10
VALUE	Ascend-Dsl-Downstream-Limit		adslcap-dn-1600000	9
VALUE	Ascend-Dsl-Downstream-Limit		adslcap-dn-1920000	8
VALUE	Ascend-Dsl-Downstream-Limit		adslcap-dn-2240000	7
VALUE	Ascend-Dsl-Downstream-Limit		adslcap-dn-2560000	6
VALUE	Ascend-Dsl-Downstream-Limit		adslcap-dn-2688000	5
VALUE	Ascend-Dsl-Downstream-Limit		adslcap-dn-3200000	4
VALUE	Ascend-Dsl-Downstream-Limit		adslcap-dn-4480000	3
VALUE	Ascend-Dsl-Downstream-Limit		adslcap-dn-5120000	2
VALUE	Ascend-Dsl-Downstream-Limit		adslcap-dn-6272000	1
VALUE	Ascend-Dsl-Downstream-Limit		adslcap-dn-640000	12
VALUE	Ascend-Dsl-Downstream-Limit		adslcap-dn-7168000	0
VALUE	Ascend-Dsl-Downstream-Limit		adslcap-dn-960000	11
VALUE	Ascend-Dsl-Downstream-Limit		adsldmt-dn-128000	121
VALUE	Ascend-Dsl-Downstream-Limit		adsldmt-dn-1280000	114
VALUE	Ascend-Dsl-Downstream-Limit		adsldmt-dn-1600000	113
VALUE	Ascend-Dsl-Downstream-Limit		adsldmt-dn-1920000	112
VALUE	Ascend-Dsl-Downstream-Limit		adsldmt-dn-2240000	111
VALUE	Ascend-Dsl-Downstream-Limit		adsldmt-dn-256000	120
VALUE	Ascend-Dsl-Downstream-Limit		adsldmt-dn-2560000	110
VALUE	Ascend-Dsl-Downstream-Limit		adsldmt-dn-2688000	109
VALUE	Ascend-Dsl-Downstream-Limit		adsldmt-dn-3200000	108
VALUE	Ascend-Dsl-Downstream-Limit		adsldmt-dn-384000	119
VALUE	Ascend-Dsl-Downstream-Limit		adsldmt-dn-4480000	107
VALUE	Ascend-Dsl-Downstream-Limit		adsldmt-dn-512000	118
VALUE	Ascend-Dsl-Downstream-Limit		adsldmt-dn-5120000	106
VALUE	Ascend-Dsl-Downstream-Limit		adsldmt-dn-6272000	105
VALUE	Ascend-Dsl-Downstream-Limit		adsldmt-dn-640000	117
VALUE	Ascend-Dsl-Downstream-Limit		adsldmt-dn-7168000	104
VALUE	Ascend-Dsl-Downstream-Limit		adsldmt-dn-768000	116
VALUE	Ascend-Dsl-Downstream-Limit		adsldmt-dn-8000000	103
VALUE	Ascend-Dsl-Downstream-Limit		adsldmt-dn-8960000	102
VALUE	Ascend-Dsl-Downstream-Limit		adsldmt-dn-9504000	101
VALUE	Ascend-Dsl-Downstream-Limit		adsldmt-dn-960000	115
VALUE	Ascend-Dsl-Downstream-Limit		adsldmt-dn-auto	100
VALUE	Ascend-Dsl-Rate-Mode		Rate-Mode-AutoBaud	1
VALUE	Ascend-Dsl-Rate-Mode		Rate-Mode-Single	2
VALUE	Ascend-Dsl-Rate-Type		Rate-Type-AdslCap	2
VALUE	Ascend-Dsl-Rate-Type		Rate-Type-AdslDmt	4
VALUE	Ascend-Dsl-Rate-Type		Rate-Type-AdslDmtCell	3
VALUE	Ascend-Dsl-Rate-Type		Rate-Type-Disabled	0
VALUE	Ascend-Dsl-Rate-Type		Rate-Type-Sdsl	1
VALUE	Ascend-Dsl-Upstream-Limit		adsldmt-up-896000	153
VALUE	Ascend-Dsl-Upstream-Limit		adslcap-up-1088000	50
VALUE	Ascend-Dsl-Upstream-Limit		adslcap-up-272000	56
VALUE	Ascend-Dsl-Upstream-Limit		adslcap-up-408000	55
VALUE	Ascend-Dsl-Upstream-Limit		adslcap-up-544000	54
VALUE	Ascend-Dsl-Upstream-Limit		adslcap-up-680000	53
VALUE	Ascend-Dsl-Upstream-Limit		adslcap-up-816000	52
VALUE	Ascend-Dsl-Upstream-Limit		adslcap-up-952000	51
VALUE	Ascend-Dsl-Upstream-Limit		adsldmt-up-1088000	151
VALUE	Ascend-Dsl-Upstream-Limit		adsldmt-up-128000	160
VALUE	Ascend-Dsl-Upstream-Limit		adsldmt-up-256000	159
VALUE	Ascend-Dsl-Upstream-Limit		adsldmt-up-384000	158
VALUE	Ascend-Dsl-Upstream-Limit		adsldmt-up-512000	157
VALUE	Ascend-Dsl-Upstream-Limit		adsldmt-up-640000	156
VALUE	Ascend-Dsl-Upstream-Limit		adsldmt-up-768000	155
VALUE	Ascend-Dsl-Upstream-Limit		adsldmt-up-800000	154
VALUE	Ascend-Dsl-Upstream-Limit		adsldmt-up-928000	152
VALUE	Ascend-Dsl-Upstream-Limit		adsldmt-up-auto	150
VALUE	Ascend-Dsl-Upstream-Limit		sdsl-1168000	5
VALUE	Ascend-Dsl-Upstream-Limit		sdsl-144000	0
VALUE	Ascend-Dsl-Upstream-Limit		sdsl-1552000	6
VALUE	Ascend-Dsl-Upstream-Limit		sdsl-2320000	7
VALUE	Ascend-Dsl-Upstream-Limit		sdsl-272000	1
VALUE	Ascend-Dsl-Upstream-Limit		sdsl-400000	2
VALUE	Ascend-Dsl-Upstream-Limit		sdsl-528000	3
VALUE	Ascend-Dsl-Upstream-Limit		sdsl-784000	4
VALUE	Ascend-FR-Link-Status-Dlci		Ascend-FR-LMI-Dlci-0	0
VALUE	Ascend-FR-Link-Status-Dlci		Ascend-FR-LMI-Dlci-1023	1023
VALUE	Ascend-Filter-Required		Required-No	0
VALUE	Ascend-Filter-Required		Required-Yes	1
VALUE	Ascend-IP-Pool-Chaining		IP-Pool-Chaining-No	0
VALUE	Ascend-IP-Pool-Chaining		IP-Pool-Chaining-Yes	1
VALUE	Ascend-IP-TOS		IP-TOS-Cost	2
VALUE	Ascend-IP-TOS		IP-TOS-Disabled	1
VALUE	Ascend-IP-TOS		IP-TOS-Latency	16
VALUE	Ascend-IP-TOS		IP-TOS-Normal	0
VALUE	Ascend-IP-TOS		IP-TOS-Reliability	4
VALUE	Ascend-IP-TOS		IP-TOS-Throughput	8
VALUE	Ascend-IP-TOS-Apply-To		IP-TOS-Apply-To-Both	3072
VALUE	Ascend-IP-TOS-Apply-To		IP-TOS-Apply-To-Incoming	1024
VALUE	Ascend-IP-TOS-Apply-To		IP-TOS-Apply-To-Outgoing	2048
VALUE	Ascend-IP-TOS-Precedence		IP-TOS-Precedence-Pri-Five	160
VALUE	Ascend-IP-TOS-Precedence		IP-TOS-Precedence-Pri-Four	128
VALUE	Ascend-IP-TOS-Precedence		IP-TOS-Precedence-Pri-Normal	0
VALUE	Ascend-IP-TOS-Precedence		IP-TOS-Precedence-Pri-One	32
VALUE	Ascend-IP-TOS-Precedence		IP-TOS-Precedence-Pri-Seven	224
VALUE	Ascend-IP-TOS-Precedence		IP-TOS-Precedence-Pri-Six	192
VALUE	Ascend-IP-TOS-Precedence		IP-TOS-Precedence-Pri-Three	96
VALUE	Ascend-IP-TOS-Precedence		IP-TOS-Precedence-Pri-Two	64
VALUE	Ascend-IPX-Header-Compression		IPX-Header-Compression-No	0
VALUE	Ascend-IPX-Header-Compression		IPX-Header-Compression-Yes	1
VALUE	Ascend-NAS-Port-Format		1_2_2	3
VALUE	Ascend-NAS-Port-Format		2_4_5_5	2
VALUE	Ascend-NAS-Port-Format		2_4_6_4	1
VALUE	Ascend-NAS-Port-Format		Unknown	0
VALUE	Ascend-Numbering-Plan-ID		ISDN-Numbering-Plan	1
VALUE	Ascend-Numbering-Plan-ID		Private-Numbering-Plan	9
VALUE	Ascend-Numbering-Plan-ID		Unknown-Numbering-Plan	0
VALUE	Ascend-PPPoE-Enable		PPPoE-No	0
VALUE	Ascend-PPPoE-Enable		PPPoE-Yes	1
VALUE	Ascend-PW-Lifetime		Lifetime-In-Days	0
VALUE	Ascend-PW-Warntime		Days-Of-Warning	0
VALUE	Ascend-Port-Redir-Protocol		Ascend-Proto-TCP	6
VALUE	Ascend-Port-Redir-Protocol		Ascend-Proto-UDP	17
VALUE	Ascend-Private-Route-Required		Required-No	0
VALUE	Ascend-Private-Route-Required		Required-Yes	1
VALUE	Ascend-Require-Auth		Not-Require-Auth	0
VALUE	Ascend-Require-Auth		Require-Auth	1
VALUE	Ascend-Route-Appletalk		Route-Appletalk-No	0
VALUE	Ascend-Route-Appletalk		Route-Appletalk-Yes	1
VALUE	Ascend-Route-IP		Route-IP-No	0
VALUE	Ascend-Route-IP		Route-IP-Yes	1
VALUE	Ascend-Route-IPX		Route-IPX-No	0
VALUE	Ascend-Route-IPX		Route-IPX-Yes	1
VALUE	Ascend-SVC-Enabled		Ascend-SVC-Enabled-No	0
VALUE	Ascend-SVC-Enabled		Ascend-SVC-Enabled-Yes	1
VALUE	Ascend-Send-Auth		Send-Auth-CHAP	2
VALUE	Ascend-Send-Auth		Send-Auth-MS-CHAP	3
VALUE	Ascend-Send-Auth		Send-Auth-None	0
VALUE	Ascend-Send-Auth		Send-Auth-PAP	1
VALUE	Ascend-Service-Type		Ascend-Service-Type-ATM	20
VALUE	Ascend-Service-Type		Ascend-Service-Type-Combinet	7
VALUE	Ascend-Service-Type		Ascend-Service-Type-EuRaw	9
VALUE	Ascend-Service-Type		Ascend-Service-Type-EuUi	10
VALUE	Ascend-Service-Type		Ascend-Service-Type-FR	8
VALUE	Ascend-Service-Type		Ascend-Service-Type-HdlcNrm	21
VALUE	Ascend-Service-Type		Ascend-Service-Type-IpFax	19
VALUE	Ascend-Service-Type		Ascend-Service-Type-MP	15
VALUE	Ascend-Service-Type		Ascend-Service-Type-MPP	5
VALUE	Ascend-Service-Type		Ascend-Service-Type-NetToNet	25
VALUE	Ascend-Service-Type		Ascend-Service-Type-None	1
VALUE	Ascend-Service-Type		Ascend-Service-Type-NotUsed	0
VALUE	Ascend-Service-Type		Ascend-Service-Type-Other	2
VALUE	Ascend-Service-Type		Ascend-Service-Type-PPP	3
VALUE	Ascend-Service-Type		Ascend-Service-Type-PseuTunPPP	18
VALUE	Ascend-Service-Type		Ascend-Service-Type-RawTcp	13
VALUE	Ascend-Service-Type		Ascend-Service-Type-Slip	4
VALUE	Ascend-Service-Type		Ascend-Service-Type-Telnet	11
VALUE	Ascend-Service-Type		Ascend-Service-Type-TelnetBin	12
VALUE	Ascend-Service-Type		Ascend-Service-Type-TermServer	14
VALUE	Ascend-Service-Type		Ascend-Service-Type-VirtualConn	16
VALUE	Ascend-Service-Type		Ascend-Service-Type-Visa2	23
VALUE	Ascend-Service-Type		Ascend-Service-Type-VoIp	22
VALUE	Ascend-Service-Type		Ascend-Service-Type-X25	6
VALUE	Ascend-Service-Type		Ascend-Service-Type-X25DChan	17
VALUE	Ascend-Session-Type		Ascend-Session-G711-Alaw	3
VALUE	Ascend-Session-Type		Ascend-Session-G711-Ulaw	2
VALUE	Ascend-Session-Type		Ascend-Session-G723	4
VALUE	Ascend-Session-Type		Ascend-Session-G723-64KPS	6
VALUE	Ascend-Session-Type		Ascend-Session-G728	7
VALUE	Ascend-Session-Type		Ascend-Session-G729	5
VALUE	Ascend-Session-Type		Ascend-Session-RT24	8
VALUE	Ascend-Session-Type		Ascend-Session-Unknown	1
VALUE	Ascend-Session-Type		Ascend-Session-Unused	0
VALUE	Ascend-Shared-Profile-Enable		Shared-Profile-No	0
VALUE	Ascend-Shared-Profile-Enable		Shared-Profile-Yes	1
VALUE	Ascend-Source-IP-Check		Source-IP-Check-No	0
VALUE	Ascend-Source-IP-Check		Source-IP-Check-Yes	1
VALUE	Ascend-TS-Idle-Mode		TS-Idle-Input	1
VALUE	Ascend-TS-Idle-Mode		TS-Idle-Input-Output	2
VALUE	Ascend-TS-Idle-Mode		TS-Idle-None	0
VALUE	Ascend-Token-Immediate		Tok-Imm-No	0
VALUE	Ascend-Token-Immediate		Tok-Imm-Yes	1
VALUE	Ascend-Tunneling-Protocol		ATMP-Tunnel	0
VALUE	Ascend-Tunneling-Protocol		VTP-Tunnel	1
VALUE	Ascend-User-Acct-Base		Base-10	0
VALUE	Ascend-User-Acct-Base		Base-16	1
VALUE	Ascend-User-Acct-Type		Ascend-User-Acct-None	0
VALUE	Ascend-User-Acct-Type		Ascend-User-Acct-User	1
VALUE	Ascend-User-Acct-Type		Ascend-User-Acct-User-Default	2
VALUE	Ascend-X25-Pad-X3-Profile		CC_SSP	4
VALUE	Ascend-X25-Pad-X3-Profile		CC_TSP	5
VALUE	Ascend-X25-Pad-X3-Profile		CRT	0
VALUE	Ascend-X25-Pad-X3-Profile		CUSTOM	11
VALUE	Ascend-X25-Pad-X3-Profile		DEFAULT	2
VALUE	Ascend-X25-Pad-X3-Profile		HARDCOPY	6
VALUE	Ascend-X25-Pad-X3-Profile		HDX	7
VALUE	Ascend-X25-Pad-X3-Profile		INFONET	1
VALUE	Ascend-X25-Pad-X3-Profile		NULL	10
VALUE	Ascend-X25-Pad-X3-Profile		POS	9
VALUE	Ascend-X25-Pad-X3-Profile		SCEN	3
VALUE	Ascend-X25-Pad-X3-Profile		SHARK	8
VALUE	Ascend-X25-Reverse-Charging		Reverse-Charging-No	0
VALUE	Ascend-X25-Reverse-Charging		Reverse-Charging-Yes	1
END-VENDOR Ascend
