#
#	Bay Networks
#	http://www.baynetworks.com/
#
#	From MegaZone <megazone@megazone.org>, as posted to the bay-isp list.
#	Modified for libradius by Alan DeKok <aland@ox.org>
#

VENDOR		Bay-Networks	1584		# now Nortel

BEGIN-VENDOR Bay-Networks
#	Bay Networks Extensions

ATTRIBUTE	Annex-Filter			28	string
ATTRIBUTE	Annex-CLI-Command		29	string
ATTRIBUTE	Annex-CLI-Filter		30	string
ATTRIBUTE	Annex-Host-Restrict		31	string
ATTRIBUTE	Annex-Host-Allow		32	string
ATTRIBUTE	Annex-Product-Name		33	string
ATTRIBUTE	Annex-SW-Version		34	string
ATTRIBUTE	Annex-Local-IP-Address		35	ipaddr
ATTRIBUTE	Annex-Callback-Portlist		36	integer
ATTRIBUTE	Annex-Sec-Profile-Index		37	integer
ATTRIBUTE	Annex-Tunnel-Authen-Type	38	integer
ATTRIBUTE	Annex-Tunnel-Authen-Mode	39	integer
ATTRIBUTE	Annex-Authen-Servers		40	string
ATTRIBUTE	Annex-Acct-Servers		41	string
ATTRIBUTE	Annex-User-Server-Location	42	integer
ATTRIBUTE	Annex-Local-Username		43	string
ATTRIBUTE	Annex-System-Disc-Reason	44	integer
ATTRIBUTE	Annex-Modem-Disc-Reason		45	integer
ATTRIBUTE	Annex-Disconnect-Reason		46	integer
ATTRIBUTE	Annex-Addr-Resolution-Protocol	47	integer
ATTRIBUTE	Annex-Addr-Resolution-Servers	48	string
ATTRIBUTE	Annex-Domain-Name		49	string
ATTRIBUTE	Annex-Transmit-Speed		50	integer
ATTRIBUTE	Annex-Receive-Speed		51	integer
ATTRIBUTE	Annex-Input-Filter		52	string
ATTRIBUTE	Annex-Output-Filter		53	string
ATTRIBUTE	Annex-Primary-DNS-Server	54	ipaddr
ATTRIBUTE	Annex-Secondary-DNS-Server	55	ipaddr
ATTRIBUTE	Annex-Primary-NBNS-Server	56	ipaddr
ATTRIBUTE	Annex-Secondary-NBNS-Server	57	ipaddr
ATTRIBUTE	Annex-Syslog-Tap		58	integer
ATTRIBUTE	Annex-Keypress-Timeout		59	integer
ATTRIBUTE	Annex-Unauthenticated-Time	60	integer
ATTRIBUTE	Annex-Re-CHAP-Timeout		61	integer
ATTRIBUTE	Annex-MRRU			62	integer
ATTRIBUTE	Annex-EDO			63	string
# Annex R18.0 software
ATTRIBUTE	Annex-PPP-Trace-Level		64	integer
ATTRIBUTE	Annex-Pre-Input-Octets		65	integer
ATTRIBUTE	Annex-Pre-Output-Octets		66	integer
ATTRIBUTE	Annex-Pre-Input-Packets		67	integer
ATTRIBUTE	Annex-Pre-Output-Packets	68	integer
ATTRIBUTE	Annex-Connect-Progress		69	integer
ATTRIBUTE	Annex-Multicast-Rate-Limit	73	integer
ATTRIBUTE	Annex-Maximum-Call-Duration	74	integer
ATTRIBUTE	Annex-Multilink-Id		75	integer
ATTRIBUTE	Annex-Num-In-Multilink		76	integer
ATTRIBUTE	Annex-Logical-Channel-Number	81	integer
ATTRIBUTE	Annex-Wan-Number		82	integer
ATTRIBUTE	Annex-Port			83	integer
ATTRIBUTE	Annex-Pool-Id			85	integer
ATTRIBUTE	Annex-Compression-Protocol	86	string
ATTRIBUTE	Annex-Transmitted-Packets	87	integer
ATTRIBUTE	Annex-Retransmitted-Packets	88	integer
ATTRIBUTE	Annex-Signal-to-Noise-Ratio	89	integer
ATTRIBUTE	Annex-Retrain-Requests-Sent	90	integer
ATTRIBUTE	Annex-Retrain-Requests-Rcvd	91	integer
ATTRIBUTE	Annex-Rate-Reneg-Req-Sent	92	integer
ATTRIBUTE	Annex-Rate-Reneg-Req-Rcvd	93	integer
ATTRIBUTE	Annex-Begin-Receive-Line-Level	94	integer
ATTRIBUTE	Annex-End-Receive-Line-Level	95	integer
ATTRIBUTE	Annex-Begin-Modulation		96	string
ATTRIBUTE	Annex-Error-Correction-Prot	97	string
ATTRIBUTE	Annex-End-Modulation		98	string

# Bay Router Specific Attributes
#
ATTRIBUTE	Annex-User-Level		100	integer	Bay-Networks
ATTRIBUTE	Annex-Audit-Level		101	integer	Bay-Networks


#	Annex Tunnel Authen Type Values

VALUE	Annex-Tunnel-Authen-Type		none		0
VALUE	Annex-Tunnel-Authen-Type		kmd5-128	1

#	Annex Tunnel Authen Mode Values

VALUE	Annex-Tunnel-Authen-Mode		none		0
VALUE	Annex-Tunnel-Authen-Mode		prefix-suffix	1

#	Annex User Server Location Values

VALUE	Annex-User-Server-Location		local		1
VALUE	Annex-User-Server-Location		remote		2

#	Annex Addr Resolution Protocol Values

VALUE	Annex-Addr-Resolution-Protocol		none		0
VALUE	Annex-Addr-Resolution-Protocol		DHCP		1

#	Annex System Disconnect Reason Values

VALUE	Annex-System-Disc-Reason		Unknown             0
VALUE	Annex-System-Disc-Reason		Line-disconnected   1
VALUE	Annex-System-Disc-Reason		Dial-failed         2
VALUE	Annex-System-Disc-Reason		WAN-manager-error   3
VALUE	Annex-System-Disc-Reason		Disconnect-reset    4
VALUE	Annex-System-Disc-Reason		Error-from-adm_notify 5
VALUE	Annex-System-Disc-Reason		Modem-down-adm_notify 6
VALUE	Annex-System-Disc-Reason		PPP-protocol-disconnect 7
VALUE	Annex-System-Disc-Reason		Inactivity-timer    8
VALUE	Annex-System-Disc-Reason		CLI-Hangup-command  9
VALUE	Annex-System-Disc-Reason		CLI-last-job        10
VALUE	Annex-System-Disc-Reason		Session-timeout     11
VALUE	Annex-System-Disc-Reason		Slave-termination   12
VALUE	Annex-System-Disc-Reason		Abnormal-termination   13
VALUE	Annex-System-Disc-Reason		DCD-wait-failed     14
VALUE	Annex-System-Disc-Reason		CLI-inactivity      15
VALUE	Annex-System-Disc-Reason		Admin-port-reset    16
VALUE	Annex-System-Disc-Reason		CLI-auth-failed     17
VALUE	Annex-System-Disc-Reason		Slave-auth-failed   18
VALUE	Annex-System-Disc-Reason		PAP-auth-failed     19
VALUE	Annex-System-Disc-Reason		CHAP-auth-failed    20
VALUE	Annex-System-Disc-Reason		Local-modem-reset   21
VALUE	Annex-System-Disc-Reason		Modem-dead          22
VALUE	Annex-System-Disc-Reason		PPP-LCP-failure     23
VALUE	Annex-System-Disc-Reason		PPP-IPCP-failure    24
VALUE	Annex-System-Disc-Reason		PPP-IPXCP-failure   25
VALUE	Annex-System-Disc-Reason		PPP-ATCP-failure    26
VALUE	Annex-System-Disc-Reason		PPP-CCP-failure     27
VALUE	Annex-System-Disc-Reason		PPP-MP-failure      28
VALUE	Annex-System-Disc-Reason		PPP-IPCP-timeout    29
VALUE	Annex-System-Disc-Reason		PPP-IPXCP-timeout   30
VALUE	Annex-System-Disc-Reason		PPP-ATCP-timeout    31
VALUE	Annex-System-Disc-Reason		PPP-CCP-timeout     32
VALUE	Annex-System-Disc-Reason		PPP-MP-timeout      33
VALUE	Annex-System-Disc-Reason		PPP-init-failure    34
VALUE	Annex-System-Disc-Reason		PPP-Unknown         35
VALUE	Annex-System-Disc-Reason		PPP-Dialback-failed 36
VALUE	Annex-System-Disc-Reason		PPP-Address-In-Use  37
VALUE	Annex-System-Disc-Reason		PPP-No-device       38
VALUE	Annex-System-Disc-Reason		PPP-Modem-hangup-rcvd  39
VALUE	Annex-System-Disc-Reason		PPP-Hangup-rcvd     40
VALUE	Annex-System-Disc-Reason		PPP-Termination-rcvd 41
VALUE	Annex-System-Disc-Reason		PPP-Kill-rcvd       42
VALUE	Annex-System-Disc-Reason		PPP-Time-rcvd       43
VALUE	Annex-System-Disc-Reason		PPP-No-memory       44
VALUE	Annex-System-Disc-Reason		PPP-Connection-Abort    45
VALUE	Annex-System-Disc-Reason		PPP-VPN-LCP-failure 46
VALUE	Annex-System-Disc-Reason		PPP-VPN-Auth-failure 47
VALUE	Annex-System-Disc-Reason		PPP-MP-invalid-port 48
VALUE	Annex-System-Disc-Reason		PPP-Invalid-device  49
VALUE	Annex-System-Disc-Reason		PPP-MMP-bundle-failure 50
VALUE	Annex-System-Disc-Reason		DVS-Registration-failure 51
VALUE	Annex-System-Disc-Reason		DVS-Home-agent-dereg    52
VALUE	Annex-System-Disc-Reason		DVS-Tunnel-no-renew 53
VALUE	Annex-System-Disc-Reason		DVS-Tunnel-expired  54

#	Annex Modem Disconnect Reason Values

VALUE	Annex-Modem-Disc-Reason			Unknown			0
VALUE	Annex-Modem-Disc-Reason			Local-disconnect	1
VALUE	Annex-Modem-Disc-Reason			CD-Timer-Expired	2
VALUE	Annex-Modem-Disc-Reason			Remote-protocol-disc	4
VALUE	Annex-Modem-Disc-Reason			Clear-down		5
VALUE	Annex-Modem-Disc-Reason			Long-Space-disconnect	6
VALUE	Annex-Modem-Disc-Reason			Carrier-Lost		7
VALUE	Annex-Modem-Disc-Reason			Modem-Retrain-Timeout	8

#	Annex Connection Progress Values

#VALUE	Annex-Connect-Progress		Progress-Unknown		2
#VALUE	Annex-Connect-Progress		Call-Is-Up			10
#VALUE	Annex-Connect-Progress		CLI-Started			40
#VALUE	Annex-Connect-Progress		LAN-Session-Is-Up		60
#VALUE	Annex-Connect-Progress		LCP-Negotiations-Allowed	61
#VALUE	Annex-Connect-Progress		CCP-Negotiations-Allowed	62
#VALUE	Annex-Connect-Progress		IPCP-Negotiations-Allowed	63
#VALUE	Annex-Connect-Progress		LCP-Is-In-Open-State		65
#VALUE	Annex-Connect-Progress		CCP-Is-In-Open-State		66
#VALUE	Annex-Connect-Progress		IPCP-Is-In-Open-State		67
#VALUE	Annex-Connect-Progress		LCP-Is-In-Closed-State		71
#VALUE	Annex-Connect-Progress		LCP-Is-In-Stopped-State		72
#VALUE	Annex-Connect-Progress		LCP-Is-In-Closing-State		73
#VALUE	Annex-Connect-Progress		LCP-Is-In-Request-Sent-State	75
#VALUE	Annex-Connect-Progress		LCP-Is-In-Ack-Recvd-State	76
#VALUE	Annex-Connect-Progress		LCP-Is-In-Ack-Sent-State	77
#VALUE	Annex-Connect-Progress		IPXCP-Is-In-Open-State		80
					
#VALUE	Annex-Multicast-Client		Multicast-No	0
#VALUE	Annex-Multicast-Client		Multicast-Yes	1

#VALUE	Annex-Inbound-Precedence		Routine			0
#VALUE	Annex-Inbound-Precedence		Priority		1
#VALUE	Annex-Inbound-Precedence		Immediate		2
#VALUE	Annex-Inbound-Precedence		Flash			3
#VALUE	Annex-Inbound-Precedence		Flash-Override		4
#VALUE	Annex-Inbound-Precedence		CRITIC/ECP		5
#VALUE	Annex-Inbound-Precedence		Internetwork-Control	6
#VALUE	Annex-Inbound-Precedence		Network-Control		7

#VALUE   Annex-Outbound-Precedence		Routine			0
#VALUE   Annex-Outbound-Precedence		Priority		1
#VALUE   Annex-Outbound-Precedence		Immediate		2
#VALUE   Annex-Outbound-Precedence		Flash			3
#VALUE   Annex-Outbound-Precedence		Flash-Override		4
#VALUE   Annex-Outbound-Precedence		CRITIC/ECP		5
#VALUE   Annex-Outbound-Precedence		Internetwork-Control	6
#VALUE   Annex-Outbound-Precedence		Network-Control		7

#VALUE	Annex-Gwy-Selection-Mode		Normal		0
#VALUE	Annex-Gwy-Selection-Mode		Backup		1
#VALUE	Annex-Gwy-Selection-Mode		Distribution	2

#VALUE	Annex-Pool-Id				Pool-One	1
#VALUE	Annex-Pool-Id				Pool-Two	2
#VALUE	Annex-Pool-Id				Pool-Three	3
#VALUE	Annex-Pool-Id				Pool-Four	4
#VALUE	Annex-Pool-Id				Pool-Five	5
#VALUE	Annex-Pool-Id				Pool-Six	6

VALUE	Annex-User-Level			Manager		2
VALUE	Annex-User-Level			User		4
VALUE	Annex-User-Level			Operator	8

VALUE	Annex-Audit-Level			Manager		2
VALUE	Annex-Audit-Level			User		4
VALUE	Annex-Audit-Level			Operator	8 

END-VENDOR Bay-Networks

#
#	Define additional Bay Networks specific values for the main
#	RADIUS dictionary
#
#	Note that '0x0630' == 1584, which is the Vendor-ID for Bay Networks.
#	Nice design, and probably the best way of adding vendor-specific
#	VALUE extensions to the standard RADIUS attributes.
#

VALUE	Service-Type		Annex-Authorize-Only		0x06300001
VALUE	Service-Type		Annex-Framed-Tunnel		0x06300002

VALUE	Acct-Status-Type	Annex-User-Reject		0x06300001
VALUE	Acct-Status-Type	Annex-Call-Reject		0x06300002
VALUE	Acct-Status-Type	Annex-IPCP-Start		0x06300003
VALUE	Acct-Status-Type	Annex-IPXCP-Start		0x06300004
VALUE	Acct-Status-Type	Annex-ATCP-Start		0x06300005
VALUE	Acct-Status-Type	Annex-Accounting-Restart	0x06300006
VALUE	Acct-Status-Type	Annex-Accounting-Shutoff	0x06300007
VALUE	Acct-Status-Type	Annex-Tunnel-Start		0x06300008
VALUE	Acct-Status-Type	Annex-Tunnel-Stop		0x06300009
VALUE	Acct-Status-Type	Annex-Tunnel-Reject		0x0630000a
VALUE	Acct-Status-Type	Annex-Tunnel-Link-Start		0x0630000b
VALUE	Acct-Status-Type	Annex-Tunnel-Link-Stop		0x0630000c
VALUE	Acct-Status-Type	Annex-MP-Start			0x0630000d
VALUE	Acct-Status-Type	Annex-MP-Stop			0x0630000e
VALUE	Acct-Status-Type	Annex-Line-Seizure		0x0630000f
VALUE	Acct-Status-Type	Annex-Rlogin-Start		0x06300010
VALUE	Acct-Status-Type	Annex-Rlogin-Stop		0x06300011

