#
# Alcatel Broadband Access Server dictionary.
#
# Version:      1.00  10-July-2002  Lasse Johnsen <lassejohnsen@bulldogcommunications.com>
#		$Id: dictionary.alcatel 28297 2009-05-08 06:10:30Z etxrab $
#

VENDOR          Alcatel         3041

#
#       Alcatel Vendor Specific Extensions
#
#
ATTRIBUTE       AAT-Client-Primary-DNS          5       ipaddr          Alcatel
ATTRIBUTE       AAT-Client-Primary-WINS-NBNS    6       ipaddr          Alcatel
ATTRIBUTE       AAT-Client-Secondary-WINS-NBNS  7       ipaddr          Alcatel
ATTRIBUTE       AAT-Client-Secondary-DNS        8       ipaddr          Alcatel
ATTRIBUTE       AAT-PPP-Address                 9       ipaddr          Alcatel
ATTRIBUTE       AAT-ATM-Direct                  21      string          Alcatel
ATTRIBUTE       AAT-IP-TOS                      22      integer         Alcatel
ATTRIBUTE       AAT-IP-TOS-Precedence           23      integer         Alcatel
ATTRIBUTE       AAT-IP-TOS-Apply-To             24      integer         Alcatel
ATTRIBUTE       AAT-MCast-Client                27      integer         Alcatel
ATTRIBUTE       AAT-Vrouter-Name                61      string          Alcatel
ATTRIBUTE       AAT-Require-Auth                62      integer         Alcatel
ATTRIBUTE       AAT-IP-Pool-Definition          63      string          Alcatel
ATTRIBUTE       AAT-Assign-IP-Pool              64      integer         Alcatel
ATTRIBUTE       AAT-Data-Filter                 65      string          Alcatel
ATTRIBUTE       AAT-Source-IP-Check             66      integer         Alcatel
ATTRIBUTE	    AAT-Qos							70	    integer         Alcatel
ATTRIBUTE	    AAT-Qoa							71	    integer         Alcatel
ATTRIBUTE	    AAT-Client-Assign-DNS			72	    integer         Alcatel
ATTRIBUTE       AAT-ATM-VPI                     128     integer         Alcatel
ATTRIBUTE       AAT-ATM-VCI                     129     integer         Alcatel
ATTRIBUTE       AAT-Input-Octets-Diff           130     integer         Alcatel
ATTRIBUTE       AAT-Output-Octets-Diff          131     integer         Alcatel
ATTRIBUTE       AAT-User-MAC-Address            132     string          Alcatel
ATTRIBUTE       AAT-ATM-Traffic-Profile         133     string          Alcatel

VALUE   AAT-MCast-Client        Multicast-No                    0
VALUE   AAT-MCast-Client        Multicast-Yes                   1

VALUE   AAT-Require-Auth        Not-Require-Auth                0
VALUE   AAT-Require-Auth        Require-Auth                    1

VALUE   AAT-Source-IP-Check     Source-IP-Check-No              0
VALUE   AAT-Source-IP-Check     Source-IP-Check-Yes             1

VALUE	AAT-FR-Direct			No								0
VALUE	AAT-FR-Direct			Yes								1

VALUE	AAT-Source-IP-Check		Source-IP-Check-No				0
VALUE	AAT-Source-IP-Check		Source-IP-Check-Yes				1

VALUE   AAT-IP-TOS              IP-TOS-Normal                   0
VALUE   AAT-IP-TOS              IP-TOS-Disabled                 1
VALUE   AAT-IP-TOS              IP-TOS-Cost                     2
VALUE   AAT-IP-TOS              IP-TOS-Reliability              4
VALUE   AAT-IP-TOS              IP-TOS-Throughput               8
VALUE   AAT-IP-TOS              IP-TOS-Latency                  16

VALUE   AAT-IP-TOS-Apply-To     IP-TOS-Apply-To-Incoming        1024
VALUE   AAT-IP-TOS-Apply-To     IP-TOS-Apply-To-Both            3072
VALUE   AAT-IP-TOS-Apply-To     IP-TOS-Apply-To-Outgoing        2048

VALUE   AAT-IP-TOS-Precedence   IP-TOS-Precedence-Pri-Normal    0
VALUE   AAT-IP-TOS-Precedence   IP-TOS-Precedence-Pri-One       32
VALUE   AAT-IP-TOS-Precedence   IP-TOS-Precedence-Pri-Two       64
VALUE   AAT-IP-TOS-Precedence   IP-TOS-Precedence-Pri-Three     96
VALUE   AAT-IP-TOS-Precedence   IP-TOS-Precedence-Pri-Four      128
VALUE   AAT-IP-TOS-Precedence   IP-TOS-Precedence-Pri-Five      160
VALUE   AAT-IP-TOS-Precedence   IP-TOS-Precedence-Pri-Six       192
VALUE   AAT-IP-TOS-Precedence   IP-TOS-Precedence-Pri-Seven     224

VALUE	AAT-Auth-Type			AAT-Auth-None					0
VALUE	AAT-Auth-Type			AAT-Auth-Default				1
VALUE	AAT-Auth-Type			AAT-Auth-Any					2
VALUE	AAT-Auth-Type			AAT-Auth-PAP					3
VALUE	AAT-Auth-Type			AAT-Auth-CHAP					4
VALUE	AAT-Auth-Type			AAT-Auth-MS-CHAP				5

VALUE	AAT-Client-Assign-DNS	DNS-Assign-No					0
VALUE	AAT-Client-Assign-DNS	DNS-Assign-Yes					1